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CENTRAL POWER DISTRIBUTION CORPORATION of A.P. Ltd.
Vidyuth Nilayam, Beside Govt. Polytechnic, ITI Road, Vijayawada-520008

e-Procurement
Tender Notice No:08/24-25 dt:  25-09-2024
CPDC of AP Ltd., intends to procure the following materials on e-procurement platform.  The details of which are as follows:

	Tender Specification No.
	Material
	Quantity

(EA)
	Date & time of downloading tender document
	Pre-Bid Meeting
	Date & time of closing bid submission
	Technical Specification bid opening date online (Technical bid stage)
	Price bid opening date on line (Financial bid stage)

	CPMPT-

   08 /24-25


	11KV 5KN Composite Silicon rubber polymer Pin Insulators with GI Pins (24mm FRP rod)
11KV 5 KN Composite Silicon Rubber Polymer Pin Insulators with GI Pins as per IEC Specification No. IEC 61109 and as per relevant IS and minimum creepage distance of 320 mm. The weight of 11KV Polymer Pin Insulators with GI Pins should be 0.9 Kg with ± 2% tolerance
	60000


	From 
  25 -09   -2024

to

upto   
10  -10 - 2024

12:00 Hrs 
	On  
 03 -10 -2024

By
 11:00 Hrs


	On   
10 -10 -2024

by 14:00 Hrs


	On
10-10 -2024
by 
16:00 Hrs


	      On
19-10 -2024
       By
13:00 Hrs



All the interested bidders may visit www.apeprocurement.gov.in  to view and download tender documents free-of-cost.


Those who are interested to submit bids will have to register in the above-mentioned site and also have to obtain Digital Certificates.  The details and procedure for obtaining digital certificates are mentioned in the website or contact the helpdesk of the site.


Bids received from the manufacturers/registered vendors of APCPDCL only will be considered.       

Phones: 08655 2955455
cgmpmm.apcpdcl@gmail.com

CHIEF GENERAL MANAGER 

P&MM: APCPDCL::VIJAYAWADA
Tender Specification No: CPMPT - 08/24-25
	Notice Inviting Tender Details

	S.No
	Description
	

	1
	Department Name
	CPDC of AP Ltd.

	2
	Office 
	Purchases & Material Management Wing, Corporate Office, CPDC of AP Ltd

	3
	Tender Number
	CPMPT - 08 /24-25

	4
	Tender Subject 
	11KV Polymer Pin Insulators with GI Pins

	5
	Delivery Schedule
	The delivery of materials shall commence in 30 days from the date of receipt of Purchase Order at the rate of 20000per month irrespective of quantity quoted or as per the requirement of APCPDCL.

	6
	Tender Type
	Open

	7
	Tender Category
	NA

	8
	Bid Security  (INR)
	2% of the Ex-works quoted value (or) Exemption of Bid Security with APCPDCL in case of Govt. firms.

	9
	Bid Security Payable to
	 EMD / Bid security shall be either online payment or in the form of Bank Guarantee.

	10
	Processing Fee (INR)
	NIL

	11
	Transaction Fee
	As per ap e-procurement portal 

	12
	Transaction Fee Payable to
	M/s. APTS, Vijayawada

	13
	Schedule Sale opening date
	25-09-2024

	14
	Pre Bid Meeting 
	03 -10 -2024 up to 11:00HRs.

	15
	Bid Submission Closing Date & time
	10-10 -2024 by 14:00Hrs.

	16
	Bid submission
	On Line

	17
	Pre-Qualification& Technical Bid Opening Date (Qualification and Eligibility Stage and Technical Bid Stage – section VI)
	10-10 -2024 by 16:00Hrs

	18
	Price Bid Opening Date

 (Financial Bid Stage) Section – VII


	On   19-10-2024 at 13:00Hrs.

	19
	Place of Tender Opening
	O/o Chief General Manager/P&MM/APCPDCL

Vidyuth Nilayam, Beside Govt. Polytechnic, ITI Road, Vijayawada-520008 Andhra Pradesh

	20
	Officer Inviting Bids/ Contact Person
	Chief General Manager/P&MM/ APCPDCL/ VIJAYAWADA


	21
	Address/E-mail id
	O/o Chief General Manager/P&MM/APCPDCL

Vidyuth Nilayam, Beside Govt. Polytechnic, ITI Road, Vijayawada-520008 Andhra Pradesh cgmpmm.cpdcl@apcpdcl.in 

	22
	Contact Details/Telephone, Fax
	Phones: 0866 2955455

	23
	Eligibility Criteria
	As per Section VI



	24
	Procedure for Bid Submission
	Bids shall be submitted online on www.apeprocurement.gov.in platform

1. The participating bidders in the tender should register themselves free of cost on e-procurement platform in the website www.apeprocurement.gov.in. 

2. Bidders can log-in to e-procurement platform in secure mode only by signing with the Digital certificates.

3. The bidders who are desirous of participating in e-procurement shall submit their technical bids, price bids as per the standard formats available at the e-market place.

4. The bidders should scan and upload the following documents in support of technical bids. The bidders shall sign on all the statements, documents certificates uploaded by him, owning responsibility for their correctness/ authenticity:  

a) Processing Fee 

b) Bid Security should be online or in the form of Bank Guarantee

 

c) “ Latest Sales Tax Clearance Certificate” 

d)  Details of previous supplies as per tender document 

e) Copies of previous supply orders in support 

    of above.

f) Turnover certificate issued by Auditor and reports on financial standing of the bidder such as profit and loss statement, balance sheets and auditors reports for the past three years etc. 

g) Duly filled and signed proforma as per Format IIIA.
h) Transaction fee payable to APTS, Vijayawada

5. The rates should be quoted in online only

	
	
	6. 

a. The bidders should upload the documents in PDF  

     format only; otherwise they are liable for rejection

b. After uploading the documents the copies of the 

    uploaded statement, certificates, documents, 

    in respect of processing fee and Bid Security      

   (except the Price bid/offer/break-up of taxes) are to 

   be submitted by the bidder to the Chief General 

   Manager/P&MM/APCPDCL so as to reach before 

   the date and time of opening of the  technical bid. 

d. Failure to furnish any of the uploaded documents, 

    certificates, before the date and time of opening of 

    technical bid will entail in rejection of the bid. 

e. The Department shall not hold any risk on account of postal delay. 

f. Similarly, if any of the certificates, documents, etc., 

    furnished by the tenderer are found to be false / 

    fabricated / bogus, the bidder will be disqualified, 

    blacklisted,  action will be initiated as deemed fit 

    and the Bid Security  will be forfeited.

7. The department will not hold any risk and responsibility regulating non-visibility of the scanned and uploaded documents.

8. The Documents that are uploaded online on e-market place will   only be considered for Technical Bid Evaluation.

9. Copies of all the uploaded statement like Previous experience, turnover details, type test reports etc. shall be notarised or attested by the gazetted  officer 

10. Important Notice to Contractors, Suppliers and Department users

(i)  In the endeavor to bring total automation of processes in e-Procurement, the Govt. has issued orders vide G.O.Ms.No. 13 dated. 5.7.2006 permitting integration of electronic Payment Gateway of ICICI/HDFC Banks with eProcurement platform, which provides a facility to participating suppliers/ contractors to electronically pay the transaction fee online using their credit cards.



	25
	Rights reserved with the Department
	APCPDCL reserves the right to accept or reject any or all of the tenders received without assigning any reasons therefore.  The APCPDCL also reserves the right to split the tender and place orders on more than one tenderer at its discretion

	26
	General Terms and Conditions
	As per tender documents.


SECTION - IIA
SALIENT FEATURES OF THE BID

Superscription on the Tender Cover




Specification No
        : CPMPT-  08/24-25
Material       : 11KV Polymer Pin Insulators with GI Pins 
Officer to whom the bid will be addressed
        : Chief General Manager/P&MM






           APCPDCL :VIJAYAWADA
Superscription on the bid cover and 

the outer envelope



:

a. Registration No. of the vendor (if any)

b. Specification No.

c. Due date and time for online submission

d. Date and time of online opening 

e. Payment of bid security



 i.   Give details: through ap eprocurement (online) online or in the form of Bank Guarantee

 



f. Whether 120 days validity offered ………(yes/no).


g. Whether bid is made accepting payment terms Clause….(yes/no).



h. Whether delivery is as per delivery schedule indicated….(yes/no)



i. Whether the sample (if specified) has been enclosed/sent…(yes/no)

Content of Bidding Documents 


The materials/equipment required, bidding procedures, and contract terms are prescribed in the bidding documents as listed below :

Section- I

: 
Notice Inviting Bids.

Section-II

:
Salient features of the Bid.

Section-III

:
Schedule of Materials  

Section-IV

:
Technical Specification

Section-V

:
General terms and conditions of contract

Section-VI

:
Qualification Requirements

Section-VII

:
Sample Forms 

Section-VIII

:
General & Eligibility

SAMPLE  FORMS

1) Bid Form and Price schedules.

2) Bid Security Form

3) Contract Form.

4) Performance Security form

5) Manufacturer’s Authorization form

6) Performance Statement

7) Details to be furnished by the Manufacturer

8) Schedule of Deviations (Technical & Commercial)

The Bidder is expected to examine all instructions, forms, terms and technical specifications in the bidding documents. Failure to furnish all information required by the bidding documents or to submit a bid not substantially responsive to the bidding documents in every respect will be at Bidder’s risk and may result in the rejection of its bid.
Deviations from standard bidding document:
ii) General terms and conditions of Contract.

iii) Technical

The above deviations super cede the existing terms of GTC and Technical specification.

CHIEF GENERAL MANAGER 

      P&MM:APCPDCL::VIJAYAWADA 

Section - IIB

The Following information shall be furnished by the bidder for technically qualifying

	Sl.No. 
	CPDCL Requirements 
	To be furnished by the bidder 

	1
	Bid Security
	through ap eprocurement (online) online or in the form of Bank Guarantee


	2
	Turnover for last 5 years 

Issued by auditor  should be enclosed in original or a copy of the same shall be attested by gazetted officer or notarized shall be enclosed

(Furnish all or any one)
	                          (In lakhs)

a) 2019-20
b) 2020-21
c) 2021-22
d) 2022-23
e) 2023-24


	3
	Previous experience year wise for last 5 years in respect of the following materials as per section –VII- schedule (f ) and the same shall be attested by gazetted officer or notarized


	2019-20
	To 
	2023-24

	4
	Delivery schedule: Commencement of supplies and (Monthly Delivery  of materials shall be furnished)   

 
	a) Supplies shall be commenced within    30 Days from the date of receipt of P.O. 

b) Monthly 20,000Nos  shall be supplied or as per the requirement of APCPDCL

	5.
	Type tests: 

Latest type test as  specified in section –IV item No.12 and Guaranteed Technical Particulars shall be furnished     
	

	7.
	APCPDCL  payment terms 


	Accepted / Not accepted 

(Delete any one )

	8.
	Tax clearance 
	Furnished / Not furnished 

(Delete any one) 

	9.
	Validity of tender for 120 days
	Accepted / Not accepted 

(Delete any one )


Note: Above information should be furnished by the tenderer for technically qualifying in the tender.  Non-furnishing of any item by the tenderer will be treated as non-responsive. 

Signature of tenderer
 SECTION – III

SCHEDULE  OF REQUIREMENTS  CPMPT  No. 08/2024-2025
	S.No
	Description
	Qty in Nos 
	Destination 



	1.
	11KV 5KN Composite Silicon rubber polymer Pin Insulators with GI Pins (24mm FRP rod)
11KV 5 KN Composite Silicon Rubber Polymer Pin Insulators with GI Pins as per IEC Specification No. IEC 61109 and as per relevant IS and minimum creepage distance of 320 mm. The weight of 11KV Polymer Pin Insulators with GI Pins should be 0.9 Kg with ± 2% tolerance
	60,000

	Gunadala

Guntur

Ongole &
CRDA




NOTE : 

1. Free at destination stores rates shall be quoted. Breakup of Ex-factory rate and freight and insurance shall be indicated. Input tax credit available to the supplier on the purchase of inputs (Raw materials) consequent to GST Act effect from 01-07-2017 shall be taken into account while quoting the prices.  The HSN code and tax rate shall be mentioned.

2. Delivery: The delivery of materials shall commence within one month from the date of purchase order. The total quantity mentioned is to be supplied as per CPDCL requirement.

3. The bidder shall quote the rate of delivery per month i.e., specific quantity (Nos.) per month.

4. The bidder should also furnish particulars/information to be furnished by the bidder enclosed to this specification. Bids not accompanied by this information are liable for rejection. 

5. Prices are Firm. 

6. Unloading charges at destination stores shall be to CPDCL account only. 
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SECTION – IV

TECHNICAL SPECIFICATION FOR THE 11KV POLYMER PIN INSULATORS WITH GI PINS

1.0. Scope

This specification covers design, manufacture, testing and supply of composite insulators for use in the 11KV overhead transmission lines and substations. 

The composite insulator will be used on lines on which the conductor will be AAA/ACSR of size up to 100 sq.mm. 

2.0. APPLICABLE STANDARDS 

2.1.
Standards

Following Indian/International Standards, which shall mean latest revision, with amendments/changes adopted and published, unless specifically stated otherwise in the specification, shall be referred while accessing conformity of insulators with these specifications. 

2.1.1 In the event of supply of insulators conforming to standards other than specified, the Bidder shall confirm in his bid that these standards are equivalent or better to those specified. In case of award, salient features of comparison between the standards proposed by the bidder and those specified in this document will be provided by the Supplier to establish equivalence. 

	Sl. No.
	Indian Standard 
	Title
	International Standard

	1.
	
	Definition, test methods and acceptance criteria for composite insulators for a.c. overhead lines above 1000V
	IEC : 61109

	2.
	IS : 731
	Porcelain insulators for overhead power lines with a nominal voltage greater than 1000V
	IEC : 60383

	3.
	IS : 2071
	Methods of High Voltage Testing 
	IEC : 60060-1

	4.
	IS : 2486
	Specification for insulator fittings for overhead power lines with a nominal voltage greater than 1000V General Requirements and Tests Dimensional Requirements Locking Devices
	IEC : 60120

IEC : 60372

	5.
	
	Thermal Mechanical Performance test and mechanical performance test on string insulator units
	IEC : 60575

	6.
	IS : 13134
	Guide for the selection of insulators in respect of polluted conditions
	IEC : 60815

	7.
	
	Characteristics of string insulator units of the long rod type
	IEC : 60433

	8.
	
	Hydrophobicity classification guide
	STRI guide 1.92/1

	9.
	
	Radio interference characteristics of overhead power lines and high-voltage equipment
	CISPR:18-2 part 2

	10.
	IS : 8263
	Methods of RI Test of HV Insulators
	IEC : 60437

	11.
	
	Standard for insulators – Composite-Distribution Dead-end type
	ANSI C29 13-2000

	12.
	IS : 4759
	Hot dip zinc coatings on structural steel & other allied products
	ISO : 1459

ISO : 1461


	13.
	IS : 2629
	Recommended Practice for Hot, Dip Galvanization for iron and steel
	ISO-1461 (E)

	14.
	IS : 6745
	Determination of weight of zinc coating on zinc coated iron and steel articles
	ISO : 1460

	15.
	IS : 3203
	Methods of testing of local thickness of electroplated coatings
	ISO : 2178

	16.
	IS : 2633
	Testing of Uniformity of coating of zinc coated articles
	

	17
	
	Standard specification for glass fiber strands
	ASTMD 578-05

	18
	
	Standard test method for compositional analysis by Thermogravimetry  
	ASTM E 1131-03

	19
	IS : 4699
	Specification for refined secondary zinc
	


The addresses of organizations who offer the above standards are given at Annexure-A

3.0. Technical Description of Composite Insulators:
3.1.
Service condition 

The polymer insulators to be supplied shall be suitable for satisfactory continuous operation under conditions as specified below:


Maximum ambient temperature 
:
500C


Minimum ambient temperature
:
-50C


Relative humidity


:
0 to 100%

3.2. Composite Insulators long rod type for tension locations and pin/ post type for suspension locations 

3.2.1. The insulators shall be suitable for 3Ph. 50Hz, effectively earthed 11KV O/H distribution system in a moderately/heavily polluted atmosphere. 

3.2.2. Bidder must be an indigenous manufacturer and supplier of composite insulators of rating 11KV or above or must have developed proven in house technology and manufacturing process for composite insulators of above rating OR posses technical collaboration/association with a manufacturer of composite insulators of rating 11KV or above. The Bidder shall furnish necessary evidence in support of the above along with the bid, which can be in the form of certification from the utilities concerned, or any other documents to the satisfaction of the owner. 

3.2.3. Insulators shall have sheds with good self-cleaning properties. Insulator shed profile, spacing, projection etc., and selection in respect of polluted conditions shall be generally in accordance with the recommendation of IEC-60815/IS : 13134.

3.2.4. The size of composite insulator, minimum creep age distance and mechanical strength along with hardware fittings shall be as follows. 
	Sl. No.
	Type of composite insulators
	Nominal system voltage KV (rms)
	Highest system voltage KV (rms)
	Visible discharge test voltage KV (rms)
	Wet power frequency withstand voltage KV (rms)
	Dry lighting Impulse withstand voltage KV (rms)
	Minimum creepage distance (mm)
	Weather Shed Dia (mm)
	Min. failing load KN
	Thickness

of Silicone Sheath

Minimum (mm)
	Bare FRP ROD Diameter(mm)

	1
	Pin Insulator
	11
	12
	9
	35
	75
	320
	95
	5
	3
	24


3.3. Dimensional Tolerance of Composite Insulators 

The tolerances on all dimensions e.g. diameter, length and creepage distance shall be allowed as follows in line with-IEC 61109 : 

± (0.04d + 1.5)mm when d(300mm

± (0.025d+6)mm when d>300mm

Where, d being the dimensions in millimeters for diameter, length or creepage distance as the case may be. 

However, no negative tolerance shall be applicable to creepage distance. 

3.4. Interchangeability 

The composite insulators including the end fitting connection shall be standard design suitable for use with the hardware fittings of any make conforming to relevant IEC/IS standards. 

3.5. Corona and RI performance 

All surfaces shall be clean, smooth, without cuts, abrasions or projections. No part shall be subjected to excessive localized pressure. The insulator and metal parts shall be so designed and manufactured that it shall avoid local corona formation and not generate any radio interference beyond specified limit under the operating conditions. 

3.6. Maintenance 

3.6.1. The composite insulators offered shall be suitable for use of hot line maintenance technique so that usual hot line operation can be carried out with ease, speed and safety. 

4.0. Technical description of composite Insulators.

4.1 Design and construction 

The composite insulator shall have a core, housing & weather shed of insulating material and steel/aluminum hardware components for attaching it to the support/conductor. 

4.1.1.
Core

It shall be a glass-fiber reinforced epoxy resin rod of high strength (FRP rod). Glass fibers and resin shall be optimized in the FRP rod. Glass fibers shall be boron free electrically corrosion resistant (ECR) glass fiber or boron free E-Glass and shall exhibit both high electrical integrity and high resistance to acid corrosion. The matrix of the FRP rod shall be Hydrolysis resistant. The FRP rod shall be manufactured through Pultrusion process. The FRP rod shall be void free. The diameter of FRP rod should be 24 mm only.  The length of FRP Rod minimum 200 mm.                                                                                                                       

4.1.2 Housing (Sheath)

The FRP rod shall be covered by a seamless sheath of a silicone elastomeric compound or silicone alloy compound of a thickness of 3 mm minimum measurable everywhere including on weathersheds. 

It should protect the FRP rod against environmental influences, external pollution and humidity. It shall be extruded or directly molded on the core and shall have chemical bonding with the FRP rod. The strength of the bond shall be greater than the tearing strength of the polymer. Sheath material in the bulk as well as in the sealing/bonding area shall be free form voids.  

4.1.3. Weather sheds 

The composite polymer weather sheds made of silicone elastomeric compound or silicon alloy shall be firmly bonded to the sheath, vulcanized to the sheath or molded as part of the sheath and shall be free from imperfections. The weather sheds should have silicon content of minimum 30% by weight. The strength of the weather sheds to sheath interface shall be greater than the tearing strength of the polymer. The interface, if any, between sheds and sheath (housing) shall be free from voids. 

4.1.4. End Fittings 

End fittings transmit the mechanical load to the core. They shall be made of spheroidal graphite cast iron, malleable cast iron or forged steel or aluminium alloy. They shall be connected to the rod by means of a controlled compression technique. The gap between fittings and sheath shall be sealed by a flexible silicone elastomeric compound or silicone alloy compound sealant. System of attachment of end fitting to the rod shall provide superior sealing performance between housing, i.e., seamless sheath and metal connection. The sealing must be moisture proof. 

The dimensions of end fittings of Insulators shall be in accordance with the standard dimensions stated in IS: 2486/IEC60120.

5.0. Workmanship

5.1. All the materials shall be of latest design and conform to the best engineering practices adopted in the high voltage filed. Bidders shall offer only such insulators as are guaranteed by them to be satisfactory and suitable for continued good service in power transmission lines. 

5.2. The design, manufacturing process and material control at various stages shall be such as to give maximum working load, highest mobility, best resistance to corrosion, good finish and elimination of sharp edges and corners.

5.3. The design of the insulators shall be such that stresses due to expansion and contraction in any part of the insulator shall not lead to deterioration. 

5.4. The core shall be sound and free of cracks and voids that may adversely affect the insulators. 

5.5. Weather sheds shall be uniform in quality. They shall be clean, sound, smooth and shall be free from defects and excessive flashing at parting lines. 

5.6. End fittings shall be free from cracks, seams, shrinks, air holes and rough edges. End fittings should be effectively sealed to prevent moisture ingress; effectiveness of sealing system must be supported by test documents. All surfaces of the metal parts shall be perfectly smooth without projecting points or irregularities, which may cause corona. All load bearing surfaces shall be smooth and uniform so as to distribute the loading stresses uniformly.  

5.7. All ferrous parts shall be hot dip galvanized to give a minimum average coating of zinc equivalent to 610 gm/sq.m. or 87(m thickness and shall be in accordance with the requirement of IS:4579. The zinc used for galvanizing shall be of purity 99.5% as per IS : 4699. The zinc coating shall be uniform, adherent, smooth, reasonably bright continuous and free from imperfections such as flux, ash rust stains, bulky white deposits and blisters. The galvanized metal parts shall be guaranteed to withstand at least four successive dips each lasting for one (1) minute duration under the standard preece test. The galvanizing shall be carried out only after any machining. 

6.0. Equipment Marking : 

6.1
Each insulator unit shall be legibly and indelibly marked with the following details as per IEC-61109 :

(a) Month & Year of manufacture

(b) Min. failing laod/guaranteed mechanical strength in kilo Newton followed by the word ‘kN’ to facilitate easy identification. 

(c) Manufacturer’s name/Trade mark. 

6.2
One 10 mm thick ring or 20mm thick spot of suitable quality of paint shall be marked on the end fitting of each composite long rod of particular strength in case of 11KV insulators for easy identification in case both types of insulators are procured by the utility. The paint shall not have any deteriorating effect on the insulator performance. 

7.0
Bid Drawings :

7.1
The Bidder shall furnish full description and illustration of the material offered. 

7.2
The bidder shall furnish along with the bid the outline drawing (3 copies) of each insulator unit including a cross sectional view of the long rod insulator unit. The drawing shall include but not be limited to the following information : 

(a) Long rod diameter with manufacturing tolerances 

(b) Minimum Creepage distance with positive tolerance 

(c) Protected creepage distance

(d) Eccentricity of the long rod unit

(i) Axial run out

(ii) Radial run out

(e) Unit mechanical and electrical characteristics

(f) Size and weight of ball and socket/tongue & clevis

(g) Weight of composite long rod units

(h) Material 

(i) Identification mark

(ii) Manufacturer’s catalogue number 


7.3
After placement of award, the supplier shall submit full dimensioned manufacturing insulator drawing containing all the details in four (4) copies to Owner for approval. After getting approval from Owner and successful completion of all the types tests, the supplier shall submit 10 more copies of the drawing to the Owner for further distribution and field use. 

7.4
After placement of award the supplier shall also submit fully dimensioned insulator crate drawing for different type of insulators for approval of the owner. 

8.0
Tests and Standards

Insulators offered shall be manufactured with the same configuration & raw materials as used in the insulators for which design & type test reports are submitted. The manufacturer shall submit a certificate for the same. The design & type test reports submitted shall not be more than 5 years old.

8.1.
Design tests 


Manufacturer should submit test reports for Design Tests as per IEC- 61109 along with the bid. Additionally following tests shall be carried out or reports for the tests shall be submitted after award of contract.

UV Test : The test shall be carried out in line with clause 7.2 of ANSI C29.13

8.2. Type Tests

8.2.1
The following type tests shall be conducted on a suitable number of individual insulator units, components, materials or complete strings and submitted along with the bid. The type test will not be later 5 years.

	Sl. No.
	Description of type test
	Test procedure/standard

	1.
	Dry lightning impulse withstand voltage test
	As per IEC 61109

	2.
	Wet power frequency test
	As per IEC 61109

	3.
	Mechanical load-time test
	As per IEC 61109

	4.
	Radio interference test
	As per IEC 61109 revised

	5.
	Recovery of Hydrophobicity test
	Annexure-B (This test may be repeated every 3 years by the manufacturer) 

	6.
	Chemical composition test for silicon content 
	Annexure-B (or any other test method acceptable to the owner) 

	7.
	Brittle fracture resistance test
	Annexure-B 


 

8.2.1. It shall be the option of the purchaser to accept the insulators based on type test reports submitted by the manufacturer. The purchaser shall be free to repeat the type test & may witness the same. 

Note : The purchaser, for the purpose of facilitating the type tests, may ask the bidders to quote test charges separately. 

8.2.2. All the type test given in clause No. 8.2 in addition to routine & acceptance test shall be carried out on insulator along with hardware fittings wherever required. 

8.3. Acceptance (sample) tests

The test samples after having with stood the routine test shall be subjected to the following acceptance test.

	a)
	Verification of dimensions 

:
IEC : 61109

	b)
	Verification of the locking system
:
IEC : 61109


(if applicable) 


	c) 
	Galvanizing test


:
IS : 2633/IS : 6745

	d)
	Verification of the specified

:
IEC : 61109

Mechanical load (if applicable)


8.4. Routine Tests

	Sl. No.
	Description
	Standard

	1.
	Identification of marking
	As per IEC : 61109

	2.
	Visual inspection
	As per IEC : 61109

	3.
	Mechanical routine test
	As per IEC : 61109


8.5. Test during manufacture

Following test shall also be carried out on all components as applicable 

	a)
	Chemical analysis of zinc used for galvanizing 

	b)
	Chemical analysis, mechanical, metallographic test and magnetic particle inspection for malleable castings. 

	c)
	Chemical analysis, hardness tests and magnetic particle inspection for forgings. 


8.6. Sample Batch for Type Testing 

8.6.1. The bidder shall offer material for sample selection for type testing only after getting Quality Assurance Programme approved by the owner. The bidder shall offer at least three times the quantity of materials required for conducting all the type tests for sample selection. The sample for type testing will be manufactured strictly in accordance with the Quality Assurance Programme approved by the owner. 

8.7. Additional Tests :

8.7.1 The purchaser reserves the right at his own expenses, for carrying out any other tests (s) of reasonable nature carried out at supplier’s premises, at site, or in any other place in addition to the aforesaid type, acceptance and routine tests to satisfy himself that the material comply with the specifications. 

8.7.2 The purchaser also reserves the right to conduct all the tests mentioned in this specification at his own expense on the samples drawn from the site at Supplier’s premises or at any other test center. In case of evidence of non compliance, it shall be binding on the part of the Supplier to prove the compliance of the items to the technical specifications by repeat tests or corrections of deficiencies or replacement of defective items, all without any extra cost to the purchaser. 

8.8. Co-ordination for Testing 

8.8.1. The supplier shall have to co-ordinate testing of insulators with hardware fittings to be supplied by other supplier and shall have to guarantee overall satisfactory performance of the insulators with the hardware fittings.

8.8.2. The bidder shall intimate the purchaser about carrying out of the type tests along with detailed testing programme at least 3 weeks advance of the scheduled date of testing during which the owner will arrange to depute his representative to be present at the time of carrying out the tests. 

8.9. Quality assurance plan 

8.9.1. The successful bidder shall submit following information to the owner :

8.9.1.1 Test certificates of the raw materials and bought out accessories.

8.9.1.2 Statement giving list of important raw materials, their grades along with names of  sub-suppliers for raw materials, list of standards according to which the raw materials are tested. List of tests normally carried out on raw materials in presence of bidder’s representative.  

8.9.1.3 List of manufacturing facilities available. 

8.9.1.4 Level of automation achieved and lists of areas where manual processing exists.

8.9.1.5 List of areas in manufacturing process, where stage inspections are normally carried out for quality control and details of such tests and inspections. 

8.9.1.6 List of testing equipment’s available with the bidder for final testing of equipment along with valid calibration reports. 

8.9.1.7 The manufacturer shall submit manufacturing Quality Plan (MQP) for approval & the same shall be followed during manufacture and testing. 

8.9.1.8 The successful bidder shall submit the routine test certificates of bought out raw materials/accessories and central excise passes for raw material at the time of inspection. 

8.10. Guarantee 

The supplier of insulators shall guarantee satisfactory performance of the insulators for a period of 18 months from the date of receipt of material at stores by the consignee in good condition. 

8.11. Test reports 

At least three copies of type test reports shall be furnished. One copy shall be returned duly certified by the owner, only after which the commercial production of the concerned material shall start. 

8.11.2 Copies of acceptance test reports shall be furnished in at least three (3) copies. One copy shall be returned duly certified by the owner, only after which the material shall be dispatched. 

8.11.3 Record of routine test reports shall be maintained by the supplier at his works for periodic inspection by the owner’s representative. 

8.11.4 Test certificates of test during manufacture shall be maintained by the supplier. These shall be produced for verification as and when desired by purchaser. 

9.0
Inspection 

9.1
The purchaser representative shall at all times be entitled to have access to the works and all places of manufacture, where insulator, and its component parts shall be manufactured and the representatives shall have full facilities for unrestricted inspection of the Supplier’s and sub-Supplier’s works, raw materials, manufacture of the material and for conducting necessary test as detailed herein. 

9.2
The material for final inspection shall be offered by the supplier only under packed condition. The owner shall select samples at random from the packed lot of carrying out acceptance tests. The lot offered for inspection shall be homogeneous and shall contain insulators manufactured in 3-4 consecutive weeks. 

9.3
The supplier shall keep the owner informed in advance of the time of starting and the progress of manufacture of material in their various stages so that arrangements could be made for inspection. 

9.4
No material shall be dispatched from its point of manufacture before it has been satisfactorily inspected and tested unless the inspection is waived off by the owner in writing. In the later case also the material shall be dispatched only after satisfactory testing specified herein has been completed. 

9.5
The acceptance of any quantity of material shall in no way relieve the Supplier of his responsibility for meeting all the requirements of the specification and shall not prevent subsequent rejection, if such material are later found to be defective. 

10.0
Packing:

10.0
All insulators shall be packed in strong corrugated box of min. 7 ply duly paletted or wooden crates. The gross weight of the crates along with the material shall not normally exceed 50 Kg to avoid handling problem.  The crates shall be suitable for outdoor storage under wet climate during rainy season. 

10.2
The packing shall be of sufficient strength to withstand rough handling during transit, storage at site and subsequent handling in the field. 

10.3
Suitable cushioning, protective padding or dunnage or spacers shall be provided to prevent damage or deformation during transit and handling. 

10.4
Al packing cases shall be marked legibly and correctly so as to ensure safe arrival at their destination and to avoid the possibility of goods being lost or wrongly dispatched on account of faulty packing and faulty or illegible markings. Each wooden case/crate/corrugated box shall have all the markings stenciled on it in indelible ink. 

10.5
The bidder shall provide instructions regarding handling and storage precautions to be taken at site. 

11.
Samples: Two samples of the above material offered against this specification shall accompany the tender and are non-returnable. The tenders received without samples are liable for rejection.
The measurements of the two samples submitted by the bidders should meet the following requirements; otherwise the bidders will be treated as non responsive.

	Sl. 
No.
	Creepage Distance (min)
	Minimum failing load
	Weight
	Dia. of bare FRP Rod

	1
	320 mm
	5 KN
	0.9 kg ± 2% tolerance
	24 mm
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A.  INTRODUCTION

1. Definitions

1.1. In this contract, the following terms will be interpreted as indicated. 

a) “The Contract” means the agreement entered into between the Purchaser and the Supplier, as recorded in the contract Form signed by the Parties, including all attachments and appendices thereto and all documents incorporated by reference there in. 

b) “The Contract Price” means the price payable to the Supplier under the Contract for the full and proper performance of its contractual obligations.

c) “The materials/equipment” means all of the equipment, machinery, and/or other materials which the Supplier is required to supply to the Purchaser under the Contract.

d) “The Services” means those service ancillary to the supply of the materials/equipment, such as transportation and insurance, and any other incidental services, such as installation, commissioning, provision of technical assistance, training, and other such obligations of the supplier covered under the contract.

e) “GTC” means the General Terms and Conditions of contract contained in the section.

f) “The Purchaser” means the organization purchasing the materials/ equipment.

g) Vendor is a supplier who has registered with the purchaser for supply of materials/equipment. 

h) “The Supplier” means the firm supplying the materials/equipment and Services under this contract.

i) “Day” means calendar day.

2. Applicability 

2.1. These General conditions of contract will apply to the extent that they are not superseded by provisions of Salient features of Bid. 

3. (a)
Standards


The materials/equipment supplied under this Contract will conform to the standards mentioned in the Technical specifications, and, when no applicable standard is mentioned, the authoritative standards appropriate to the materials/equipment i.e., BIS, such standards will be the latest. All material will be of the best class and will be capable of satisfactory operation under tropical conditions without distortion or deterioration. 

(b)
Interchangeability 


All similar materials and removable parts of similar equipment will be interchangeable with each other. A specific confirmation of this should be furnished in the bid. 

4. Scope of Work


This specification covers design manufacture, testing and delivery FADS (Free at Destination stores) of the materials described at Section ‘Schedule of Material of Volume-I’ and ‘Technical Specification Section of Volume-I’. 















5. Eligible Bidders  


Manufacturers/Vendors who have registered themselves with DISCOM for supply of the material / equipment listed in Section No. IV, of Bid specification and meeting the qualification requirements described at section VI only need quote. 
B. THE BIDDING DOCUMENTS

6. Contents of Bidding Document 

6.1. The material/equipment required, bidding procedures, and contract terms are prescribed in the bidding documents as listed below.

1. Notice Inviting Bid

2. Salient Features of the Bid

3. General terms and conditions of contract

4. Schedule of requirements (Delivery Schedule)

5. Technical specification

6. Qualification Requirements

7. Bid Form and Price Schedules

8. Bid Security

9. Performance Security Form

10.  Schedule of Deviations 

6.2. The Bidder is expected to examine all instructions, forms, terms and Technical specifications in the bidding documents. Failure to furnish all information required by the bidding documents or to submit a bid not responsive to the bidding documents in every respect will be at Bidder’s risk and may result in the rejection of its bid.

7. Clarification of Bidding Documents 

Clarification of Bidding Documents : A prospective Bidder requiring any clarification of the bidding documents may notify the purchaser in writing or by cable (hereinafter, the term cable is deemed to include telex and fax) 

at the Purchaser’s address. The Purchaser will respond in writing to any request for clarification of the bidding documents, which it receives no later than fifteen (15) days prior to the deadline for the submission of bids. 

8. Amendment to Bidding Documents 

8.1. At any time prior to the deadline for submission of bids, the purchaser, for any reason, whether at its own initiative or in response to a clarification requested by a prospective Bidder, may modify the bidding documents by amendment.

8.2. All such amendments also would be made available on the e-Procurement Portal and such amendments will be binding on the respective Bidders.

8.3. In order to allow prospective bidders reasonable time in which to take the amendment into account in preparing their bids, the purchaser, at its discretion, may extend the deadline for the submission of bids.

C. PREPARATION OF BIDS

9. Language of Bid


The bid prepared by the Bidder including all correspondence and documents relating to the bid exchanged by the Bidder and the Purchaser, will be in English only.

10. Cost Associated with Bidding 

The Bidder will bear all costs associated with the preparation and submission of its bid, and the purchaser, will in no case be responsible or liable for those costs, regardless of the conduct or outcome of the bidding process.

11. Documents constituting the Bid 

11.1 The bid prepared by the Bidder will comprise the following components:

i.           Bid security Paid 
ii.           A Bid Form and Price Schedule completed in accordance with

Clause No.12 and 13.

iii.           Documentary evidence establishing in accordance with Clause

No.19 that the Bidder is eligible to bid and is qualified to perform the contract if its bid is accepted.

iv.           Documentary evidence establishing that the Materials / equipment and ancillary services to be supplied by the Bidder are   as   per   the   Technical   specification   of   the   bidding documents; and

v.          Bid Security in accordance with Clause No.20.

vi.          Tax clearance  certificate 

vii.          Schedule of Deviations

i. Commercial 

ii. Technical

All the Schedules will be duly filled but not necessary in the sheets attached to  the  specification  unless  full  details  required  in  the  schedules  are furnished the Bids will be liable for rejection.

12. Bid Form 

12.1. The Bidder will complete the Bid form and the appropriate Price Schedule (only for online submission) furnished in the bidding documents, indicating the materials/equipment to be supplied, a brief description of the materials/equipment, quantity and prices.

13. Bid Prices 

13.1. The prices quoted will be Firm. Bids will be called for with prices FADS inclusive of packing and forwarding, F&I, GST and other legally permissible duties and levies wherever applicable, handling charges to cover the transport by road from destination railway station to site/stores, unloading at destination and insurance (transit and storage at site for 45 days). Unloading at destination stores is to CPDCL’s account. 

13.2. Even though composite price is given the break-up for all the duties, taxes, freight, insurance, packing and forwarding etc., will be furnished. 

13.3. It is the responsibility of the Bidder to inform himself of the correct rates of duties and taxes leviable on the materials at the time of bidding. 

13.4. The proforma credit available to the bidder on the purchases of inputs (raw materials) consequent to the introduction of “GST’ may be taken into account while quoting the prices. 

13.5. The Bidder will indicate on the appropriate Price Schedule the unit prices (where applicable) and total bid price of the materials/equipment it proposes to supply under the contract. Any alternative offers shall be indicated only in the price schedule.

The price of the materials/ equipment quoted Ex-Works and ther duties and sales and other taxes payable on the finished materials/ equipment with individual breakup for taxes and duties, packing and forwarding, freight and insurance etc., 

14. Variable prices & price variation provision both on positive side and negative side may be made for the equipment/material such as Transformers, Cables, Conductors & Winding Wires etc., where the variation is expected to be significant.

14.1. Wherever prices quoted are not firm (prices FADS, ED., ST., freight, Insurance, packing, forwarding and other legally permissible duties and levies will be given separately. 

14.2. Quotations will be with prices subject to adjustment up or down as per specific variation formula with reference to the base prices of major raw materials/ components involved which will be detailed in the bid along with the respective percentage costs in the composite price for the finished goods. 

14.3. Whenever IEEMA price variation formula is applicable, the Bidder may quote according to IEEMA formula in force at the time of bidding which will remain the same through out the execution and completion of the order. 

14.4. The quoted prices will be on FADS basis inclusive of transit cum 45 days storage insurance inclusive of all taxes and duties.

14.5. The prices of raw-materials/components will be those at which Bidder actually purchases from their principal suppliers (whose names will be invariably stated) and will not be the landed cost at the Bidder’s work including transport or any other charges. The basic price of raw materials so quoted will remain unaltered during the period of validity of bid as well as during the execution of contract.

14.6. Where IEEMA formula is not applicable and where the raw materials such as Steel, Aluminium, Zinc, Lead and Copper are involved the SAIL/TISCO/ MUKUND price of steel for Zinc and Copper as published by IEEMA and the BALCO/HINDALCO/NALCO/MALCO price of aluminium will be applicable for price variation. The base and final prices/indices will correspond to the same manufacturers. 

14.7. In case of conductors, where the bidder makes his own arrangements to get the properzi rod made out of Aluminium, Ingot, the price of Properzi Rod as prevailing at the time of the bidder obtaining the ingot from the primary producers will only be taken into consideration for arriving at the price variation claims irrespective of whatever expenditure the bidder might have incurred in getting the ingot converted into Properzi Rod. 

14.8. In case where variable prices are quoted, if complete information as above is not given, the bid is liable for rejection.

Irrespective of the increase in the prices of raw materials the price variance (increase) will be limited to maximum of 50% ceiling on positive side and no ceiling on negative side over the original quoted price. 

Note :
In case of Transformers, conductors and LT AB Cables, the above Clause 14.8 may be read as follows: “In case where variable prices are quoted, if complete information as above is not given, the bid is liable for rejection. Price variation on the raw materials as per IEEMA /CACMAI formulae over the original quoted price will be allowed for procurement of power and Distribution Transformers of various capacities, conductors and LT AB Cables”, 
14.9. If the date of delivery as defined in the P.V. formula is beyond the contracted delivery date, the scheduled delivery date or the actual delivery date which ever is advantageous to the purchaser will form the basis for calculation of price variation.

14.10. Not withstanding the formula applicable for regulating the price variation, if at any time any documentary evidence proof or certificate in regard to the price variation bills is required by the purchaser, the bidder will have to furnish the same to the purchaser.

14.11. The price for inland transportation, insurance, packing and forwarding and other local costs incidental to delivery of the materials/ equipment to their final destination,

15. Taxes and Duties

15.1      A bidder will be entirely responsible for quoting the correct taxes and duties, other local taxes or levies if any, license fees, etc., he has to incur until completion of the contract. For the purpose of evaluation the bidder should clearly indicate the GST and any other taxes and levies payable in the respective columns provided in the price schedule. Failure to furnish the details as prescribed in the price schedule will be loaded as indicated in the evaluation criteria. If any exemptions on taxes and duties, shall furnish proof of exemption certificate.

15.2      If the rates of statutory levies assumed by the bidder are less than the actual rates prevailing at the time of bidding, the purchaser will not be responsible for such errors. If the rates of statutory levies assumed by the Bidder are later proved to be higher than the actual/correct rates prevailing at the time of bidding, the difference will be passed on to the credit of the purchaser. 

16. Statutory Variations 


Any variation up or down in statutory levy or new levies introduced after Signing of the contract under this specification will be to the account of APCPDCL provided that in cases where delivery schedule is not adhered to by the supplier and there are upward variation/revision after the agreed delivered date the supplier will bear the impact of such levies and if there is downward variation/revision the APCPDCL will be given credit to that extent.  

17. Bid Currencies 


Prices will be quoted in Indian Rupees; and will be paid in Indian Rupees only.
18. Quantity to quote 


Bidder will quote a minimum quantity of at least 20% of the total quantity indicated in the bid specification. Offers less than the minimum prescribed are liable for rejection. 

19. Documents Establishing Bidder’s Eligibility and qualifications 


The Bidder will furnish, as part of its bid, documents establishing the Bidder’s eligibility to bid  and its qualifications to perform the contract if its bid is accepted. 


The documentary evidence of the bidders qualifications to perform the contract of its bid is accepted will establish to the purchaser’s satisfaction. 

a) that the Bidder has the financial, technical, and production capability necessary to perform the contract ;

b) that the Bidder meets the qualification criteria listed in Section IV. In addition the Bidder may furnish full particulars regarding supply of the material in question made so far to APCPDCL during the last 5 years and other reputed utilities.  

19.1. Documents Establishing materials/ equipment conformity to Bidding documents 


The Bidder will furnish as part of its bid, documents establishing conformity to the bidding documents of all materials/equipment and services, which the Bidder proposes to supply under the contract. 


The documentary evidence of conformity of the materials/equipment and the services to bidding documents may be in the form of literature, drawings, and data, and will consist of :  

a) A detailed description of the essential technical and performance characteristics of the materials/equipment. 

b) The bidder should specifically mention about furnishing the test certificates and a specimen form of test certificate should be furnished along with the bid. 

c) A list giving full particulars, including available sources and current prices of spare parts, special tools etc., necessary for the proper and continuing functioning of the materials/equipment following commencement of the use of the materials/ equipment by the purchaser; and

d) An item-by-item commentary on the purchaser’s Technical specifications demonstrating substantial responsive-ness of the materials/equipment and services to those specifications, or a statement of deviations and exceptions to the provisions of the technical specifications.


For purpose of the commentary to be furnished pursuant to above, the Bidder will note that standards for workmanship, material, and equipment, as well as references to brand names or catalogue numbers designated by the Purchaser in its Technical Specifications, are intended to be descriptive only and not restrictive. The Bidder may substitute alternative standards, brand names, and/or catalogue numbers in its bid, provided that it demonstrates to the Purchaser’s satisfaction that the substitutions ensure substantial equivalence to those designated in the Technical Specifications.

20. Bid Security 

20.1 All bids will be secured by an amount specified by the purchaser as noted below: 

Earnest money deposit / Bid Security:

2% of the total Ex-works value of the material offered

EMD / Bid security shall be either online payment or in the form of Bank Guarantee.

Bid Security will be forfeited and the vendor black listed if:

1.  Bidder withdraws  his  bid  or  alters  the  prices  before  the  expiry  of validity.

2.  Bidder withdraws his bid after its acceptance. In such a case his vendor registration will also be cancelled.

3.  Bidder  violates  any  of  the  provisions  of  these  regulations  or  the conditions of the Bid issued by the Competent Authority.

4.  Samples are not furnished within the time limit prescribed.

20.2. The fact of having enclosed bid security by On Line payment along with the bid should be clearly super scribed on the bid envelope
20.3. Submission of BID SECURITY by way of cheque, cash, money order, cash deposit will not be accepted and will be considered as disqualification. 

20.4. This clause is deleted.

20.5. Payment of BID SECURITY will be waived at the discretion of the APCPDCL in the case of fully owned Government undertaking of the Central or State Government. Such undertakings should immediately apply and obtain exemption before submitting their bids. They need only refer to the details of such exemption in their Bids. Exemption accorded by any organization other than APCPDCL will not be considered.

20.6. Deleted.
20.7. Requests for exemption from payment of BID SECURITY will not be entertained in any case.

20.8. Any bid not secured as above will be rejected by the Purchaser.

20.9. Unsuccessful Bidder’s Bid Security will be discharged or returned as promptly as possible but not later than thirty (30) days after the expiration of the period of bid validity prescribed by the purchaser. 

20.10. The successful Bidders’ Bid security will be discharged upon the bidder signing the contract.

20.11. The Bid Security may be forfeited 

(a) If a Bidder

i. Withdraws its bid or alters its prices during the period of bid validity specified by the Bidder on the Bid Form, or

ii. Does not accept the correction of errors pursuant to clause No. 30.2; or

iii. Offers post Bid rebates, revision or deviations in quoted prices and/ or conditions or any such offers which will give a benefit to the Bidder over others will not only be rejected outright but the original Bid itself will get disqualified on this account and the Bidder’s BID SECURITY will be forfeited. 

(b)
In the case of a successful Bidder, if the Bidder fails :

i. To sign the contract in accordance with clause No.38

ii. To furnish performance security in accordance with clause No. 39. 

20.12 In cases where the Bid cover contains superscription of having furnished Bid Security by way of DD but if the same is not found within, such Bids will be rejected and bidder will run the risk of being banned.

21. Period of validity of Bids

21.1 Bids will remain valid for the period of Ninety (120) days from the date of bid  opening prescribed by the purchaser. A bid valid for a shorter period will be rejected.


The bidders should clearly super scribe on the sealed envelopes of the bids about the validity. Bids not containing superscription of validity will be rejected and returned unopened.

21.2 In exceptional circumstances, the purchaser may solicit the Bidder’s consent to an extension of the period of validity. The request and the responses there to will be made in writing (or by cable). The Bid Security provided under clause No. 20 will also be suitably extended. A Bidder may refuse the request without forfeiting its Bids Security. 

22 Tax Clearance certificates 

22.1 Copies of Income Tax, Sales Tax and Turnover Tax certificates for the latest period from the appropriate authority will invariably be enclosed to the bid in the case of proprietary or partnership for it will be necessary to produce the certificate/certificates for the proprietor or proprietors and for each of the partners as the case may be. If the Bidder has already produced the certificate during the calendar year in which the bid is made, it will be sufficient, if particulars are given.

23 Service Conditions 

23.1. The equipment/materials offered will be entirely satisfactory for operation under the climatic conditions indicated below :

a) Maximum ambient air temperature (in shade)

450C

b) Maximum ambient air temperature (under sun)

500C

c) Maximum daily average ambient air temperature

350C

d) Maximum yearly average ambient air temperature
300C

e) Maximum humidity





100%

f) Altitude above M.S.L.




upto 1000 M

g) Average No. of thunder storm days per annum

50

h) Average NO. of dust storm days per annum

Occasional

i) Average No. of rainy days/annum



90

j) Average Annual Rain fall




925 mm

k) Normal tropical monsoon period



4 months

l) Maximum wind pressure




150 Kg/sq.m.

23.2. Due consideration will be given to any special devices or attachments put forward by the Bidder which are calculated to enhance the general utility and the safe and efficient operation of the equipment /materials.

24. Format and Signing of bid.

24.1. The Bidder will prepare an original and one more copies of the bid, clearly marking each “ORIGINAL BID” and “COPY OF BID”, as appropriate. In the event of any discrepancy between them, the original will govern.

24.2. The original and the copies of the bid will be typed and will be signed by the Bidder or a person or persons duly authorized to bind the Bidder to the contract. The person or persons signing the bid will initial all pages of the bid, except for printed literature. 

24.3. Any interlineations, erasures, or overwriting will be valid only if they are initialed by person or persons signing the bid. 

D.
SUBMISSION OF BIDS

25. Sealing and Marking of Bids.

25.1. The Bidder will seal the original and each copy of the bid in separate envelopes, duly marking envelopes as “ORIGINAL: and the “COPY”. The envelopes will then be sealed in an outer envelope. 

25.2. The inner and outer envelopes will ;

a) Be addressed to the purchaser,

25.3. The sealed cover as well as the outer envelope should be super scribed as follows. 

a) Registration No. of the vendor

b) Bid Enquiry No.

c) Due date and time for submission

d) Date and time for opening

e) Payment of Bid Security


i) Give details : through apeprocurement (online) online or in the form of Bank Guarantee

 



   Name of the Bank:_____________________



   Amount__________________________

f) Whether 120 days validity offered _______ Yes/No

g) Whether the quotation is made accepting payment terms clause ---- Yes/No

h) Whether the delivery is as per delivery schedule indicated --- Yes/No.

i) Whether the sample (if specified) has been enclosed/sent --- Yes/No

25.4. Deleted.

25.5. The Bidder will invariably complete the bid in full.

25.6. Deleted.

25.7. Dleleted.

25.8. Deleted.

25.9. Deleted.

26. Deadline for submission of Bids

26.1. Bids together with modifications if any, or other withdrawals must be received by the Purchaser not later than the deadline for submission of bids specified in the salient features of the Bid. 

26.2. The purchaser may, at its discretion, extend this deadline for the submission of bids by amending the bidding documents in which case all rights and obligations of the purchaser and Bidders previously subject to the deadline will thereafter be subject to the deadline as extended.

27. Late Bids

27.1. Deleted.

27.2. Modification and withdrawal of Bids


The Bidder may modify or withdraw its bid after the bid’s submission, provided that written notice of the modification, including substitution or withdrawal of the bids, is received by the purchaser prior to the deadline prescribed for submission of bids. 

E.
OPENING AND EVALUATION OF BIDS

28. Opening of Bids by the Purchaser

28.1.  In case of procurement of materials through e-Procurement portal Bids will be   opened on-line, on the specified day and time indicated in the bid specification. 

28.2. Deleted. 

28.3. Deleted.

29. Clarification of Bids

29.1. During evaluation of the bids, the purchaser may, at its discretion, ask the bidder for a clarification of its, bid. The request for clarification and the response will be in writing, and no change in the prices or substance of the bid will be sought, offered, or permitted. 

30. Preliminary Examination

30.1. The purchaser will examine the bids to determine whether they are complete, whether any computational errors have been made, whether required sureties have been furnished, whether the documents have been properly signed, and whether the bids are generally in order.

30.2. Arithmetical errors will be rectified on the following basis.   If there is a discrepancy between the unit price and the total price that is obtained by multiplying the unit price and quantity, the unit price will prevail, and the total price will be corrected. If the Supplier does not accept the correction of the errors, its bid will be rejected, and its Bid Security may be forfeited.  If there is a discrepancy between words and figures, the amount in words will prevail.  If the supplier does not accept the correction of the errors, its bid will be rejected and its Bid Security may be forfeited. In case of a discrepancy between soft copy and hard copy, the entries in hard copy will prevail. 

30.3. The purchaser may waive any minor informality, nonconformity, or irregularity in bid which does not constitute a material deviation, provided such waiver doesn’t prejudice or affect the relative ranking of any bidder. 

30.4. Prior to the detailed evaluation, the purchaser will determine the substantial responsiveness of each bid to the bidding documents. For purposes of these clauses, a substantially responsive bid is one, which conforms to all the terms and conditions of the bidding documents without material deviations. Deviations from, or objections or reservations to critical provisions, such as those concerning Bid Security, and Taxes and Duties will be deemed to be a material deviation. The purchaser’s determination of a bid’s responsiveness is to be based on the contents of the bid itself without recourse to extrinsic evidence.

30.5. If a bid is not substantially responsive, it will be rejected by the purchaser and may not subsequently be made responsive by the bidder by correction of the nonconformity.

31. Evaluation and Comparison of Bids

31.1. The purchaser will evaluate and compare the bids, which have been determined to be substantially responsive.

31.2. The purchaser’s evaluation of a bid will take into consideration one or more of the following factors.


All the bids, which are opened, read out and considered for evaluation will be checked for qualification requirements in respect of the technical and commercial aspects. Such of the bids, which do not meet the qualification requirements, will not be evaluated further. The bid is to be checked for its conformity to the technical specification. If it does not meet the technical specification, the Bid will not be evaluated further. However, if in the opinion of the purchaser the bidder has offered equipment/material better than the technical specification the same may be considered. The bid may be rejected for the following reasons :

1. Not in the prescribed form

2. Insufficient bid security or bid not accompanied by the required bid security.

3. Bids not properly signed

4. The bidder is a vendor who is banned from further business transactions and the period of ban is still in force. 

5. Bid received after the due date and time.

6. The bid is through telegram or fax.

7.    Bids submitted not as per measuring units mentioned in the tender document. 

For example:  If  the unit of measurement in tenders is in Kilolitres (KL)  & if the bidder has quoted his rate for Litres with the same unit of measurement in kilo Litres (KL), then the bidder has to be disqualified as the bidder quoted rate is too low for Kilo Litre which is impossible to supply at that rate.

· Further, the purchaser may enquire from the bidder in writing for any clarification of the bid. The response of the bidder will also be in writing. However no change in the prices or substance of the bid will be sought, offered or permitted. 

· Bids will be examined for completeness and for any computational errors.

· Arithmetical errors will be rectified on the following basis.

· Where there is a discrepancy between the unit price and total price, the unit price will prevail and the total price will be corrected accordingly.

· Where there is a discrepancy between words and figures, the amount in words will prevail.

· If the bidder does not attest any overwriting in the price column such Bids will be rejected. 

· Failure on the part of the bidder to agree to the above corrections will result in rejection of his offer and forfeiture of his bid security.

· It will be ensured that the required sureties have been furnished and that the documents have been properly signed.

· The purchaser’s evaluation of a bid shall take into consideration one or more of the following factors. 

a) Delivery schedule offered in the bid;

b) Deviations in payment schedule from that specified in the general terms and conditions of the contract and technical deviations.

c) The cost of components, mandatory spare parts, and service;

d) The availability of spare parts and after-sales services for the equipment offered in the Bid;

e) The projected operating and maintenance costs during the life of the equipment;


The performance and productivity of the equipment offered; Other specific criteria indicated in the Bidding documents.


In addition the purchaser’s evaluation of a bid will take into account the net landed cost of the material at the final destination. For the purpose of evaluation net landed cost is arrived at by adding all elements of the basic price, allowable discount, any other levies, packing and forwarding, freight charges, insurance (transit & storage) as quoted by the bidder, interest on advance if any, unloading at final destination, erection, servicing and other charges exclusive of GST as called for.   


In addition any variation up or down in taxes and duties/new levies introduced  subsequent to bid opening and before award will be considered for comparison purposes.

The following criteria may be adopted for taxes and duties for evaluation.

a) It is the responsibility of the bidder to quote all taxes and duties correctly without leaving any column unfilled (see samples form 1). Where taxes and duties are not applicable the bidder should enter “NA”. If no duty/tax is leviable the same may be entered as “NIL”. If any column is left blank or filled vaguely like “as applicable”, the same will be loaded with the maximum of the other eligible Bids.

b) Where there is an exemption of GST the documentary evidence to that effect will be enclosed by the supplier.

c) The bidders for supply and works shall invariably possess the TIN Number and PAN Number for the bids above Rs.5.00 lakhs and this must be verified before entering into contract.

*
Prior to detailed evaluation, the responsiveness of each bid will be determined. A substantially responsive bid is one that conforms to al the terms and conditions of the bidding documents without materials deviations. For this purpose superscription, qualification requirement, bid security, validity, delivery, payment term, price schedule, taxes and duties will be deemed to be the critical provisions and deviations in any one of these items will be deemed to be a material deviation. 


The purchaser may waive any minor informality, non-conformity or irregularity in the bid which does not constitute a material deviation, provided such waiver does not affect the relative ranking of any bidder. The purchaser will clearly indicate in the bid specification the methodology for evaluation of bids.

a) Bid price, which will include all, costs of manufacture and services at manufacturing places as well as, Transportation to destination stores, packing and forwarding, insurance and all taxes and other legally permissible duties & levies payable.  

b) Delivery schedule offered in the bid.

c) Deviations in payment schedule from that specified in the general terms and conditions of the contract.

d) The cost of components, mandatory spare parts, and service.

e) The availability of spare parts and after-sales services for the equipment offered in the Bid;

f) The projected operating and maintenance costs during the life of the equipment.

g) The performance and productivity of the equipment offered; and/or

h) Other specific criteria indicated in the Bid specification.

31.3(a)
The purchaser’s evaluation of a bid will take into account the Net Landed Cost of the material at destination stores inclusive of all taxes and duties quoted by the Bidder. It is the responsibility of the bidder to quote all taxes and duties correctly without leaving any column unfilled. Where not applicable the column may be filled as “NA”. If no duty/tax is leviable the same may be filled as “NIL”. If any column is left blank the same is loaded with maximum of other eligible Bids. If any overwriting is not attested by the bidder in the price schedule such Bids will be rejected.

(b)
Any statutory variations of taxes and duties and new levies imposed after opening of the bid and before award of the contact will be taken into consideration for the purpose of evaluation.

31.4. A substantially responsive bid is one, which conforms to all the terms and conditions of the bidding documents without material deviations. For this purpose superscription, qualification requirement, bid security, validity, delivery, payment term, price schedule, submission of type test certificates (as per Clause 4 section-VI), taxes and duties will be deemed to the critical provisions and deviations in any one of these things will be deemed to be a material deviation.

32. Contacting the Purchaser.

32.2  From the time of the opening to the time of contract award, if any Bidder wishes  to contact the purchaser on any matter related to the bid, it should do so in writing.

32.3  Any effort by a bidder to influence the purchaser in its decisions on bid evaluation, bid comparison, or contract award will result in the rejection of the Bidder’s bid.

F. AWARD OF CONTRACT 

33 Post Qualification

33.1 In the absence of pre-qualification, the purchaser will determine to its satisfaction whether the Bidder that is selected as having submitted the lowest evaluated responsive bid is qualified to perform the contract satisfactorily. 

33.2 The determination will take into account the Bidder’s financial, and production capabilities. It will be based upon an examination of the documentary evidence of the Bidder’s qualification submitted by the Bidder, as well as such other information as the Purchaser deems necessary and appropriate.

34 Award Criteria:

Negotiations will only be held with responsive L1. Negotiations can also be   held with all the responsive firms to explore the possibility of a further reduction in price where the rates are considered to be too high with reference to estimated price or updated prices of the past orders. 

If the L1 bidder quoted price is reasonable then the full quantity could be ordered on L1.

Considering other than L1 would be limited to the following cases only. 

a. When it is clearly felt that L1 cannot supply the total quantity in the required time schedule or in the opinion of the purchaser it is undesirable to depend on one supplier. Then 50% of the quantity (or) quantity quoted by L1 whichever is less should be given to L1. Balance quantity may be distributed among other bidders   at the discretion powers of CMD.

b. In all these above cases, quantity could be distributed to all those agreeing to the lowest rate offered by the suppliers during negotiations or any other acceptable rates. 

However, it is not binding on DISCOM to accept the lowest or any other Bid and allocation of quantities. It reserves the right to place orders on different Bidders.

34.1      If the tenders are cancelled CMD has got powers to procure on nomination

Basis (or) in open market.  

35. Purchaser’s Right to Vary Quantities at the time of Award

35.1. The purchaser reserves the right at the time of contract award to increase or decrease the quantity of materials/equipment and services originally specified in the Schedule of Requirements without any change in unit price or other terms and conditions.

35.2. The purchaser reserves the right to vary the ordered quantity by +/- 50% during the execution of the contract.

36. Purchaser’s right to accept any bid and to reject any or all Bids

36.1. The Purchaser reserves the right to accept or reject any bid, and to annual the bidding process and reject all bids at any time prior to contract award, without thereby incurring any liability to the affected Bidder or Bidders or any obligation to inform the affected Bidder or Bidders.

37. Notification of Award

37.1. Prior to the expiration of the period of bid validity, the purchaser will notify the successful bidder in writing by registered letter or by cable, to be confirmed in writing by registered letter, that its bid has been accepted.

37.2. The notification of award will constitute the formation of the contract. 

37.3. Upon the successful Bidder’s furnishing of the performance security, the purchaser enters into contract with successful Bidder/Bidders. The purchaser will notify each unsuccessful Bidder and will discharge its bid Security. 

38. Signing of contract


The Purchaser notifies the successful Bidder that its bid has been accepted. Within 30 days (thirty days) of receipt of notification of award of contract, the successful Bidder will sign and date the contract. Failure to comply with this stipulation will entail cancellation of the contract besides forfeiture of the bid security.

39. Performance Security

●      The  successful  bidder  /  bidders  will  submit  security  for     proper fulfillment of the contract and such security will be for an   amount of 10% (ten percent) of the contract value (or)  as per govt.  order.

●
This performance security will be furnished within 15 days of receipt of the notification of contract award and should cover a period of 6 months beyond the warranty period. Failure to comply with this stipulation will entail canceling of the contract besides forfeiture of the bid security and cancellation of the vendor’s registration.

●
The performance security will be in the form of banker’s cheque crossed Demand Draft from a nationalized bank / pay order/ cash/ On-Line transfer / individual / Permanent Bank Guarantee.

●
The   purchaser   will   discharge   the   performance   security   after completion of the contract and within 6 months of the expiry of the warranty.

●
The Bank Guarantees may be obtained from the State Bank of India or its Associate Banks / Nationalized Banks/Scheduled Bank
    The Bank Guarantees towards performance security shall be submitted as follows:

Performance Bank Guarantee (Transformers & VCBs):

(i) Local Manufacturers:

5% Performance Guarantee of the contract value.








(Or)

2% of the contract value to be submitted initially for a period of 3 years with an undertaking to extend for the balance period of the warranty, prior to 3 months of its expiry plus deduction of 5% of the each bill till 3% of the contract value is deducted towards performance guarantee.

 (or)

A Permanent Performance Bank Guarantee (PPBG) for a value of Rs. 20 Crore.

(ii) For Others:

10% of the contract value (As per the existing norms) 

a) Performance Bank Guarantee (Other Materials):

(i) Local Manufacturers:

5% Performance Guarantee of the contract value.

(Or)

2% of the contract value to be submitted initially for a period of 3 years with an undertaking to extend for the balance period of the warranty, prior to 3 months of its expiry plus deduction of 5% of the each bill till 3% of the contract value is deducted towards performance guarantee.

(or)

A Permanent Performance Bank Guarantee (PPBG) for a value of Rs. 1.0 Crore. 

(ii) For Others:

10% of the contract value (As per the existing norms).

b) Definition of Local Equipment Manufacturing Unit:

As per the Policy of Govt. of Andhra Pradesh.

c) Permanent Performance Bank Guarantee (PPBG) for a value of                       Rs.20 Crore for the existing / ongoing works for the contractor who comes forward with acceptance.

d) Exemptions will be given in case of Payment of performance security based on the recommendation made by the SPC for special cases.

            Failure of the successful Bidder to comply with the above requirement will entail cancellation of the award and forfeiture of the Bid Security.

40. Corrupt or Fraudulent Practices 


It is essential that the purchaser as well as Bidder/supplier/contractor for the purposes of this provision, the terms set forth below as follows :

(i) “Corrupt practice” means the offering, giving, receiving or soliciting of any thing of value to influence the action of a public official in the procurement process or in contract execution, and

(ii) “Fraudulent Practice” means a misrepresentation of facts in order to influence a procurement process or the execution of a contract to the detrimental of the purchaser, and includes collusive practice among Bidders (prior to or after bid submission) designed to establish bid prices at artificial non-competitive levels and to deprive the purchaser of the benefits of free and open competition;

(iii) Will reject a proposal for award if it determines that the Bidder recommended for award has engaged in corrupt or fraudulent practices in competing for the contract in question;

(iv) Will declare a firm ineligible, either indefinitely or for a stated period of time, to be awarded a contract if it at anytime determines that the firm has engaged in corrupt or fraudulent practices in competing for, or in executing, a contract.

41. Use of contract Documents and Information

41.1. The supplier will not, without the purchaser’s prior written consent, disclose the contract, or any provision thereof, of any specification, plan, drawing, pattern, sample, or information furnished by or on behalf of the purchaser in connection therewith, to any person other than a person employed by the Supplier in the performance of the contract. Disclosure to any such employed person will be made in confidence and will extend only so far as may be necessary for purposes of such performance.

41.2. The supplier will not, without the purchaser’s prior written consent, make use of any document or information except for purpose of performing the contract.

41.3. Any document, other than the contract itself, will remain the property of the purchaser and will be returned (in all copies) to the purchaser on completion of the supplier’s performance under the contract if so required by the purchaser.

41.4. The supplier will permit the purchaser or his authorized representative to inspect the supplier’s accounts and records relating to the performance of the supplier and to have them audited by auditors appointed by the supplier.

42. Patent Rights

42.1. The Supplier will indemnify the Purchaser against all third-party claims of infringement of patent, trademark, or industrial design rights arising from use of the materials/ equipment of any part thereof. 

43. Places/ Locations:

43.1. Particulars of site location and nearest rail heads to which the equipments/ material have to be supplied will be given to successful bidders.

44. Delivery

44.1. Delivery period will be reckoned from the date of signing of the contract. The delivery quoted will be firm, definite, unconditional and on the basis of receipt of materials at destination in good condition without any bearing on the procurement of raw materials or any similar prerequisites. The commencement date and date of delivery will be indicated. The preferred delivery time, which is the essence of this specification, is indicated in the schedule. Final deliveries are however, subject to confirmation at the time contract. Delay in delivery of materials FADS (Free at destination store) due to non-availability of railway booking non-allotment of wagons and any such reasons will not be considered. It is the responsibility of the supplier to make alternative arrangements for transporting the materials by road or rail so as to see that the material reaches the destination within the stipulated period. The purchaser reserves its right to defer the delivery date at any time after orders are placed without any change in the conclusion of contract other condition supply. The delivery period, which will be reckoned from the date of the contract, will 
be guaranteed under penalty as in clause 61. 

45. Inspections and Tests

(i) The supplier will keep the purchaser informed in advance of the time of the starting and the progress of manufacture of equipment in its various stages so that arrangement could be made for inspection. The accredited representative of the APCPDCL will have access to the supplier’s or his subcontractor’s work at any time during working hours for the purpose of inspecting the materials during manufacturing of the materials/equipment and testing and may select test samples from the materials going into plant and equipment. The supplier will provide the facilities for testing such samples at any time including access to drawings and production data at no charge to purchaser. As soon as the materials are ready the supplier will duly send intimation to APCPDCL by Regd. Post and carry out the tests in the presence of representative of the APCPDCL.

(ii) The APCPDCL may at its option get the materials inspected by the third party if it feels necessary and all inspection charges in this connection will be borne by the supplier.

(iii) The dispatches will be affected only if the test results comply with the specification. The dispatches will be made only after the inspection by the APCPDCL officer is competed to the APCPDCL satisfaction or such inspection is waived by the competent authority.

(iv) The acceptance of any quantity of materials will in no way relieve the supplier of its responsibility for meeting all the requirements of this specification and will not prevent subsequent rejection if such materials are later found to be defective.

(v) The supplier will give 15 days advance intimation to enable the purchaser depute his representative for witnessing the acceptance and routine tests. 

(vi) Should any inspected or tested materials/equipment fail to conform to the specification, the purchaser may reject the materials and supplier will either replace the rejected materials or make alternations necessary to meet specifications requirements free of costs to the purchaser.

(vii) In  the  case  of  transformers,  instrument  transformers  and  meters

inspection will be conducted every year, for the first 5 years on a 2% sample of the quantities supplied. Samples will be collected at random at field or stores to establish  that  the  guaranteed  technical  parameters  are  as  per  the submitted  bid  by  the  supplier.  In  the  case  of  non-adherence,  the purchaser may take suitable action on the supplier including cancellation of vendor registration and banning further dealings, depending on the gravity of the deviation. These random inspections may be entrusted to a third party.

46. Name Plate :


Equipment should be provided with name plate giving full details of manufacture, capacities and other details as specified in the relevant ISS or other specification stipulated. The P.O. No. and date, year of supply, period of warranty and the words “APCPDCL” must be etched on the name plate.

47. Packing

47.1. The Supplier will provide such packing of the materials/ equipment as is required to prevent their damage or deterioration during transit to their final destination, as indicated in the Contract. The packing will be sufficient to withstand, without limitation, rough handling during transit and exposure to extreme temperatures, salt and precipitation during transit, and open storage. Packing case size and weights will take into consideration, where appropriate, the remoteness of the materials/equipment final destination and the absence of heavy handling facilities at all points in transit.

47.2. The packing, making, and documentation and outside the packages will comply strictly with such special requirements as will be expressly provided for in the contract and in any subsequent instructions ordered by the purchaser. The supplier will be required to make separate packages for each consignee, each package will be marked on three sides with proper paint/indelible ink with the following ;

1. Contract Number

2. Supplier’s name

3. packing list reference number

47.3. The supplier, whenever dispatches material to a destination should prepare the following information in the form of packing slip in quadruplicate and send the same to the consignee and obtain his acknowledgement. The consignee will return to the supplier one copy of the packing slip with his remarks. The proforma of packing slip will be as follows. 

PACKING SLIP

1. Contract No. & Date

2. Quantity allotted to the stores and rate applicable

3. Quantity so far supplied to the stores and the rate applied.

4. Quantity now supplied and the rate applied. 

5. Total quantity supplied under the contract with rates supplied.

6. Programme for supplying the balance quantity to the stores.

48. Delivery Documents 

48.1. Delivery of the materials/equipment will be made by the supplier in accordance with the terms specified in the contract.


The latest test certificates containing the result of the tests as per the relevant ISS or other specification stipulated must be submitted to the Chief General Manager and got approved by him.

48.2. Documents to be submitted by the supplier are specified as under …

(i)
Insurance certificate ;

(ii)
Supplier’s certificate certifying that the defects if any pointed out during inspection have been rectified (3 copies).

(iii)
Manuals in six sets and one set of reproducible drawings. 


The purchaser will receive the above documents soon after the dispatch of materials and if not received, the supplier will be responsible for any consequent expenses.

49. Insurance

49.1. The materials/equipment  will be fully insured against loss or damage incidental to manufacturer or acquisition, transport, storage and delivery in the manner specified in the contract and also storage for 45 days at the destination site or stores before taking into stock. 


Insurance will be in an amount equal to 100% FADS value of material/equipment on all risks basis.  The policy will have a provision for extension to cover further storage, if necessary, at the destination site or stores at the purchaser’s cost.  The insurance beneficiary shall be APCPDCL . 

50. Transportation

50.1. The Supplier is required under the Contract to transport the materials/ equipment to a specified place of destination defined as normally the district stores, transport to such place of destination, including insurance and storage, will be arranged by the supplier, and the related costs will be included in the contract price only.

51. Incidental Services

51.1. The Supplier may be required to provide any or all of the following services, including additional services, if any

a) Performance or supervision of on-site assembly and/or start-up of the supplied materials/equipment.

b) Furnishing of tools required for assembly and/or maintenance of the supplied materials/equipment ;

c) Furnishing of a detailed operations and maintenance manual for each appropriate unit of the supplied materials/equipment. 

d) Performance or supervision or maintenance and/or repair of the supplied materials/equipment, during warranty period, provided that this service will not relieve the supplier of any warranty obligations under this contract ; and

e) Training of the purchaser’s personnel, at the supplier’s plant and/or on-site, in assembly, startup, operation, maintenance, and/or repair of the supplied materials/equipment.

52. Spare Parts

52.1. The supplier may be required to provide any or all of the following materials, notifications, and information pertaining to spare parts manufactured or distributed by the supplier. 

a) Such spare parts as the purchaser may choose to purchase from the supplier, provided that this selection will not relieve the supplier of any warranty obligations under the contract; and 

b) In the event of termination of production of the spare parts;

c) Advance notification to the purchaser of the impending termination.

d) Time to permit the purchase to procure needed requirement; and following such termination, furnishing at no cost to the purchaser, the blueprints, drawings, and specifications of the spare parts; if requested. 

53. Warranty

53.1. The supplier will warrant for the satisfactory functioning of the material/ equipment as per specification for a minimum period of 18 months from the date of receipt of the material/equipment in good condition except for transformers, Energy meters and VCBs etc. and for transformers, meters and VCBs the warranty shall be as mentioned in Section ‘Technical Specifications.  

53.2. The Supplier warrants that the materials/equipment supplied under the contract are new, unused, of the most recent or, current models, and that they incorporate all recent improvements in design and materials unless provided otherwise in the contract. The supplier further warrants that all materials/equipment supplied under this contract will have no defect, arising from a design and/or materials as required by the purchaser’s specifications or from any act of omission of the supplier, that may develop under normal use of the supplied materials/equipment. 

53.3. All the material will be of the best class and will be capable of satisfactory operation in the tropics under service conditions indicated in clause 23.1 without distortion or deterioration. No welding filing or plugging of defective parts will be permitted, unless otherwise specified, they will conform to the requirements of appropriate Indian, British or American Standards. (Where a standard specification covering the material in question has not been published, the standards of the American Society for testing of materials should be followed). 

53.4. The entire designs and constructions will be capable of withstanding the severest stresses likely to occur in actual service and of resisting rough handling during transport.

53.5. Unless otherwise specified the warranty period will be 18 months from the date of acceptance of the materials/ equipment. The supplier will, in addition, comply with the performance guarantees specified under the contract. If, for reasons attributable to the supplier, these guarantees are not attained in whole or in part, the supplier will at its discretion either, make such changes, modifications, and/or additions to the materials/equipment or any part thereof as may be necessary in order to attain the contractual guarantees specified in the contract at its own cost and expense and to carry out further performance tests as per the relevant standards. 

53.6. The purchaser will promptly notify the supplier in writing of any claims arising under this warranty.

53.7. “Upon receipt of such notice, the Supplier will within 30 days repair or replace the defective materials/ equipment or pars thereof, free of cost at the ultimate destination. The supplier will take over the replaced parts/ materials/equipment at the time of their replacement. No claim whatsoever will lie on the purchaser for the replaced parts/materials/equipment thereafter. In the event of any correction of defects or replacement of defective material during the warranty period, the warranty for the corrected/replaced material will be extended to a further period of 12 months. 

53.8. If the Supplier, having been notified, fails to remedy the defect(s) within the above period, the purchaser may proceed to take such remedial action as may be necessary, at the supplier’s risk and expense duly deducting the                                                                     expenditure from subsequent bills/bank guarantee and without prejudice to any other rights which the purchaser may have against the supplier under the contract.

54. Payment

54.1. 100% payment will be arranged on or after 30 days from the date of Form-13, i.e., receipt of material/ equipment in good condition at the destination stores or after submission of bills in complete shape with other necessary enclosures whichever is later duly transferring the said amount to the bank account of the supplier by the purchaser bank. The supplier will have to predefine the bank details while entering into contract.  

54.2. The 100% payment mentioned above is subject to submission of performance security as per clause 39 by the supplier.

54.3. The supplier should invariably submit test certificates and other documents, the purchaser specifies as soon as dispatch is made so that they can be checked and approved well in advance.

54.4. The performance guarantee to be executed in accordance with this specification will be furnished on a stamp paper of value Rs. 100/-. The Bank Guarantee will be extended if required suitably. In accordance with the provisions of clause No. 39.

54.5. If the supplier has received any over payments by mistake or if any amounts are due to the APCPDCL due to any other reason, when it is not possible to recover such amounts under the contract resulting out of this specification, the APCPDCL reserves the right to collect the same from any other amount and/or Bank Guarantees given by the company due to or with the APCPDCL. 

54.6. When the supplier does not at any time, fulfill his obligations in replacing/ rectifying etc., of the damaged/defective materials in part or whole promptly to the satisfaction of the APCPDCL Officers, the APCPDCL reserves the right not to accept the bills against subsequent dispatches made by the supplier and only the supplier will be responsible for any demurrages, wharf ages or damage occurring to the consignments so dispatched.  

55. Prices

55.1. Prices charged by the supplier for materials/equipment delivered and service performed under the contract will not vary from the prices quoted by the supplier in its bid, with the exception of any price adjustment authorized in the contract. 

56. Change Orders

56.1. The purchaser may at any time, by a written order given to the Supplier make changes within the general scope of the contract in any one or more of the following

a) Drawings, designs  or specifications, where materials/equipment to be furnished under the contract are to be specifically manufactured for the purchaser;

b) The method of shipment or packing;

c) The place of delivery; and /or

d) The services to be provided by the supplier.

57. Contract Amendments 

57.1. No variation in or modification of the terms of the Contract will be made except by written amendment by the purchaser and accepted by the supplier.

58. Assignment 

58.1. The Supplier will not assign, in whole or in part, its obligations to perform under this contract, except with the purchasers, prior written consent.

59. Delay in Supplier’s performance

59.1. Delivery of the materials/equipment will be made by the Supplier in accordance with the time schedule prescribed by the purchaser in the schedule of Requirements. 

59.2. If at any time during performance of the contract, the supplier should encounter conditions impeding timely delivery of the materials/equipment, the Supplier will promptly notify the purchaser in writing of the fact of the delay, its likely duration and its cause(s). As soon as practicable after receipt of the supplier’s notice, the purchaser will evaluate the situation and may at its discretion extend the suppliers time for performance, with or without liquidated damages, in which case the extension will be ratified by the parties by amendment of the contract.

59.3. Except as provided under “force majeure” clause a delay by the Supplier in the performance of its delivery obligations will render the supplier liable to the imposition of liquidated damages unless an extension of time is agreed upon without the application of liquidated damages. 

60. Penalty for delay in supplies


The time for and the dates for delivery mentioned in the contract will be deemed to be the essence of the contract subject to “force majeure” clause No. 64, if the supplier failed to deliver any or all of the materials /equipment or to perform the services within the periods(s) specified in the contract, the purchaser will, without prejudice to its other remedies under the contract, deduct from the contract price, as liquidated damages, a sum equivalent to 0.5% per week on the undelivered portion subject to a maximum of 5% of the cost of materials undelivered in time. Once the maximum is reached the purchaser may consider termination of the contract. 


The date of Form-13 ie., the date of receipt of materials at destination stores in good condition will be taken as the date of delivery. Materials / Equipment which are not of acceptable quality or are not confirming to the specification would be deemed to be not delivered. For penalty, the number of days would be rounded of to the nearest week and penalty calculated accordingly.

The penalty specified above will be levied and would be adjusted against subsequent pending bills. Penalty will not be levied in case of delay due to Force majeure events. 


The penalty specified above will be levied and would be adjusted against subsequent pending bills.

Any failure on the part of new vendors for a second time would cause them to be removed from the list of registered vendors.

61. Termination for Default. 

61.1. The Purchaser, without prejudice to any other remedy for breach of Contract, by written notice of default sent to the Supplier, may terminate this Contract in whole or in part.

i. If the Supplier fails to deliver any or all of the Materials / equipment within the period(s) specified in the Contract, or within any extension thereof granted by the Purchaser.

ii. If the Supplier, fails to perform any other obligation(s) under the Contract.

iii. If the Supplier, in the judgment of the Purchaser has engaged incorrupt or fraudulent practices in competing for or in executing the Contract.

61.2. In the event the Purchaser terminates the Contract in whole or in part, the Purchaser may procure, upon such terms and in such manner, as it deems appropriate, Materials / equipment or services similar to those undelivered, and the Supplier will be liable to the Purchaser for any excess costs for such similar materials / equipment or Services. However, the Supplier will continue performance of the Contract to the extent not terminated.

62. Termination for Insolvency

62.1. The Purchaser may at any time terminate the Contract by giving written notice to the Supplier if the Supplier becomes bankrupt or otherwise insolvent. In this event, termination will be without compensation to the supplier, provided that such termination will not prejudice or not affect any right of action or remedy, which has accrued or will accrue thereafter to the Purchaser.

63. Termination for Convenience 

63.1. The Purchaser, by written notice sent to the Supplier, may terminate the Contract, in whole or in part, at any time for its convenience. The notice of termination will specify the termination is for the Purchaser’s convenience, the extent to which performance of the supplier under the Contract is terminated, and date upon which termination becomes effective.

63.2. However the Materials / equipment that are complete and ready for shipment within thirty (30) days after the supplier’s receipt of notice of termination will be accepted by the Purchaser at the Contract terms and prices.

64. Force Majeure

64.1. The Supplier will not be liable for forfeiture of its performance security, penalty for late delivery, or termination for default if and to the extent that its delay in performance or other failure to perform its obligations under the contact is the result of an event of Force majeure.

64.2. For purpose of this clause, “Force Majeure” means an event beyond the control of the Supplier and not involving the Supplier’s fault or negligence and not foreseeable. Such events may include, but are not restricted to, wars or revolutions fires, floods, epidemics, quarantine restrictions, and freight embargoes.

64.3. If a Force majeure situation arises, the supplier will promptly notify the purchaser in writing of such condition and the cause thereof. Unless otherwise directed by the Purchaser in writing, the Supplier will continue to perform its obligations under the contract as far as is reasonably practice, and will seek all reasonable alternative means for performance not prevented by the Force Majeure event.

No price variance will be allowed during the period of Force Majeure. 

65. Settlement of Disputes

65.1. If any dispute or difference of any kind whatsoever will arise between the purchaser and the Supplier in connection with or arising out of the contract, the parties will make every effort to resolve amicably such dispute or difference by mutual consultation. 

65.2. If, after thirty (30) days the parties have failed to resolve their dispute or difference by such mutual consultation, then either the purchaser or the supplier may give notice to the other party of its intention to commence arbitration, as hereinafter provided, as to the matter in dispute, and no arbitration in respect of this matter may be commenced unless such notice is given. 

65.3. Any dispute of difference in respect of which a notice of intention to commence arbitration has been given in accordance with this clause will be finally settled by arbitration. Arbitration may be commenced prior to or after delivery of the materials/ equipment under the contract. 

65.4. Arbitration proceedings will be conducted in accordance with the following rules of procedure. The dispute resolution mechanism will be as follows :

a) In the case of a dispute or difference arising between the purchaser and a supplier relating to any matter arising out of or connected with this agreement, such dispute or difference will be settled in accordance with the Arbitration and Conciliation Act. 1996. The Arbitral Tribunal will consist of three Arbitrators one each to be appointed by the Purchaser and the supplier the Third Arbitrator will be chosen by the two arbitrators so appointed by the parties and will acts as Presiding Arbitrator. In case of failure of the two Arbitrators appointed by the parties to reach upon a consensus within period of 30 days from the appointment of the Arbitrator appointed subsequently, the Presiding Arbitrator will be appointed by The Institution of Engineers (India).

b) If one of the Parties fails to appoint its Arbitrator in pursuance of Sub-Clause (a) within 30 days after receipt of the notice of the appointment of its Arbitrator by the Institution of Engineers (India), will appoint the Arbitrator. A certified copy of the order of the Institution of Engineers (India), making such an appointment will be furnished to each to the parties.  

c) Arbitration proceedings will be held at purchaser’s Headquarters, and the language of the Arbitration proceedings and that of all documents and communication between the parties will be English. 

d) The decision of the majority of Arbitrators will be final and binding upon both parties. The cost and expenses of Arbitration proceedings will be paid as determined by the Arbitral Tribunal. However, the expenses incurred by each party in connection with the preparation, presentation etc., of its proceedings as also the fees and expenses paid to the Arbitrator appointed by such party or on its behalf will be borne by each party itself. 

e) Where the value of the contract is Rs. one crore and below, the disputes or differences arising will be referred to the Sole Arbitrator. The sole arbitrator should be appointed by agreement between the parties; failing such agreement, by the appointing authority namely The Institution of Engineers (India).

65.5. Notwithstanding any reference to arbitration herein

a) The parties will continue to perform their respective obligations under the contract unless they otherwise agree; and

b) The Purchaser will pay the supplier any amount due to the supplier. 

66. Jurisdiction

66.1. All and any disputes or differences arising out of or touching this contract will be decided by the courts or Tribunals situated in Purchaser’s Headquarters only. No suit or other legal proceedings will be instituted elsewhere.

67. Notices

67.1. Any notice given by one party to the other pursuant to this Contract will be sent to the other party in writing or by cable, telex, or facsimile and confirmed in writing to the other party’s address.

67.2. A notice will be effective when delivered or on the notice’s effective date, whichever is later.

68. Foreign Exchange  

68.1. No Foreign Exchange is available or expected for this purchaser. Offers which do not require release of F.E. or procurement of import license by APCPDCL only will be considered. Where some of the components are to be imported the manufacturer will have to make their own arrangements for import license etc., and should not look for any assistance from APCPDCL.

SECTION – VI 

                          QUALIFICATION  REQUIREMENTS

1.
The   bidder   should   be   a   manufacturer / registered vendor who   must   have   designed, manufactured, tested and supplied to power utilities at least 40% of the quoted quantity of the goods / equipment of same or higher voltage/capacity class indicated in the “Schedule of Requirement” in one continuous period of 12 months and its financial turnover during any one year of the last five years should have been equal or more than 100% value of the material now quoted.




 For this purpose Order completion certificates, Performance certificates issued by the utility not below the rank of General Manger / Superintending Engineer, Stores material receipt acknowledgement (Form-13) will be considered.
At least 20% of same or similar material offered against this Specification should be in successful operation since 2 years as on the date of opening of the Bid for major materials like PTRs, DTRs, VCBs, Energy Meters of all types, Instrument Transformers, Over Head Conductors / Cables, UG Cables and other equipment on the material supplied during last seven years  (and)
 since 1 year for all other materials on the material supplied during last  five years.

The requirement of 20% Performance on the same or similar material offered against the specification is based on the material to be procured 
For this purpose Performance certificates issued by the utility not below the rank of General Manger / Superintending Engineer during the last seven/five years as on the date of opening of the Bid will only be considered.
2.
The bidder should furnish the information on all past supplies  and satisfactory performance in proforma under Form 6.

3.       All bids submitted will also include the following information:

i.
Copies of original documents defining the constitution or legal status, place of registration and principle place of business of the company or firm or partnership, etc.,

ii.       The bidder should furnish a brief write-up, backed with 

 adequate data,explaining his available capacity and experience (both technical and commercial)  for  the  manufacture  and  supply  of  the  required equipment within the specified time of completion after meeting all their current commitments.

iii.      The bidder should clearly confirm that all the facilities exist in his factory for inspection and testing and these will be made available to the purchaser or his representative for inspection.
iv.      Reports on financial standing of the Bidder such as profit and loss statement, balance sheets and auditor’s report for the past three years, bankers certificates etc.

4.
The bidder will furnish Type Test Results. The type tests must have been conducted on the material offered  as per the relevant  IS in recognized NABL Accredited Laboratory as per the latest revision of the Technical Specification and the date of Type tests will not be later than 5 years subject to no alteration in the design.  The Bids received without type test reports will be treated as Non-Responsive. If any change in design was made latest type tests shall be furnished along with approved drawings.


The validity of Type tests shall be as per recommendations of Minister of Power, CEA, Govt. of India from time to time and same will be specified in the bid document.

5.       Even though the bidder meets the above qualifying criteria, they are subject

to be disqualified if they have…

a.
made misleading or false representations in the forms statements and attachments submitted in proof of qualification requirements and / or

b.
record  of poor  performance  such  as  not  properly  completing  the contract, inordinate delays in supply completion, litigation history or financial failure etc.

6.
Not withstanding anything stated above the purchaser reserves the right to assess bidder’s capability and capacity to performs the contract should circumstances warrant such an assessment in the overall interest of the purchaser.

7. The bidder must furnish the details as indicated in FORM No. 7 of Section-III (i.e., Details to be furnished by the manufacturer). 

8. The relation ship with any TRANSCO/DISCOM employee must be disclosed by the bidders.

9. “Any bidder/company blacklisted by any A.P. Power utility will be disqualified”.

CHIEF GENERAL MANAGER 

P&MM:APCPDCL::VIJAYAWADA 
SECTION – VII

SAMPLE FORMS

1. BID FORM AND PRICE SCHEDULES


Date:…………


TO : (Name and Address of Purchaser)


Gentlemen and /or Ladies :


Having examined the Bidding documents, the receipt of which is hereby duly acknowledged, we, the undersigned, offer to supply and  deliver. _____________ (Description of Materials/ equipment) in conformity with the said bidding documents for the sum of ________ (total bid amount in words and in figures) or such other sums as may be ascertained in accordance with the schedule of prices attached herewith and made part of this Bid.


We undertake, if our Bid is accepted, to deliver the materials/equipment in accordance with the delivery schedule specified in the Schedule of Requirements. 


We agree to abide by this Bid upto ____________ (for the Bid validity period) specified in clause and it will remain binding upon us and may be accepted at any time before the expiration of that period. 


Until a formal contact is prepared and executed, this Bid, together with your written acceptance thereof and your notification of award, will constitute a binding contract between us.


We understand that you are not bound to accept the lowest or any bid you may receive.


We certify/confirm that we comply with the eligibility requirements as per clause of the bidding documents.


Dated this ………… day of ………. 2024


________________________________


________________________________


(Signature)







(In the capacity of)


Duly authorized to sign bid for and on behalf of



2) PRICE SCHEDULE

	Sl No
	Name of material
	Quantity required
	APCPDCL delivery Schedule
	Quantity offered by the Bidder
	Whether firm 

	1
	2
	3
	4
	5
	6


	Free at Destination Stores
	GST
	Any other tax/duties (Specify)
	Unit 

Price 
	Discount if any
	Total price Rs. Ps.
	Remarks

	Ex-Works price per unit
	Packing and Forwarding Freight and Insurance
	
	
	
	
	
	

	7
	8
	9
	10
	11
	12
	13
	14


Note      :
Columns 1 to 4 to be filled in by the purchaser and the remaining columns are to be filed by the Bidder. 

Signature of the Bidder

2. BID SECURITY FORM
Whereas.  .............. (hereinafter called "the Bidder") has submitted its Bid dated (date  of  submission  of  bid)  for  the  supply  of.    ....................(name  and  /or description of the Materials / equipment) (hereinafter called "the Bid").

KNOW ALL PEOPLE by these presents that WE.  .............(name of bank) having our registered office at. ...........(address of bank) (hereinafter called "the Bank"), are bound unto.  ...............(name of Purchaser) (hereinafter called "the Purchaser") in the sum of                        for which payment well and truly to be made to the said Purchaser, the Bank binds itself, its successors, and assigns by these presents. Sealed with the Common Seal of the said Bank this          day of             20 .

THE CONDITIONS of this obligation are:

1.       If the Bidder

a)  withdraws its Bid during the period of bid validity specified by the

Bidder on the Bid Form; or

b)  does not accept the correction of errors in accordance with the Bid

Specification, or

2.       If the Bidder, having been notified of the acceptance of its bid by the

Purchaser during the period of bid validity;

(a)
fails or refuses to furnish the performance security, in accordance with the Bid Specification.

(b)     fails or refuses to execute the Contract Form if required; or

We undertake to pay the Purchaser up to the above amount upon receipt of its first written demand, without the Purchaser having to substantiate its demand, provided that in its demand the Purchaser will note that the amount claimed by it is due to it, owing to the occurrence of one or both of the two conditions, specifying the occurred condition or conditions.

This guarantee will remain in force up to and including forty five (45) days after

…………….(Specification Date) the period of the bid validity, and any demand in

respect thereof should reach the Bank not later than the above date.

 ....................

 (Signature of the Bank)

NOTE:        This will be executed on a Rs.100/- non-judicial stamp paper issued

by a scheduled Bank.

3. CONTRACT FORM

THIS AGREEMENT made the _______ day of _______ 20     between ________ (Name of Purchaser) on one part and _________ (Name of Supplier) on the other part :

WHEREAS the Purchaser invited bids for certain materials/ equipment and ancillary service viz.,………………………………………………………………………………………………

…………………. (Brief description of materials/equipment and Services) and has accepted a bid by the Supplier for the supply of those materials/equipment and services in the sum of ……………… (Contract Price in Words and Figures) (hereinafter called “ the contract price”).

NOW THIS AGREEMENT WITNESSTH AS FOLLOWS

1. In this agreement words and expressions will have the same meanings as are respectively assigned to them in the Conditions of Contract referred to.

2. The following documents will be deemed to form and be read and constructed as part of this Agreement, viz.,

a) The Bid Form and the price schedule submitted by the Bidder;

b) The Schedule of Requirements;

c) The Technical Specifications;

d) The General Conditions of Contract;

e) The Purchaser’s Notification of Award.

3. In consideration of the payments to be made by the Purchaser to the Supplier as hereinafter mentioned, the supplier hereby covenants with the Purchaser to provide the materials/equipment and services and to remedy defects therein in conformity in all respects with the provisions of the contract.

4. The Purchaser hereby covenants to pay the Supplier in consideration of the provision of the materials/equipment and services and the remedying 

of defects therein, the Contract Price or such other sum as may become payable under the provisions of the Contract at the times and in the manner prescribed by the Contract. 

Brief particulars of the materials/equipment and services which will be supplied/provided by the Supplier are as under :

	Sl. NO.
	Brief Description of materials/ Equipment and services
	Quantity to be supplied 
	Unit Price

Rs.
	Total Price Rs.
	Delivery Terms

	
	
	
	
	
	

	
	
	
	
	
	


TOTAL VALUE : (Rupees _____________________________________ only)
DELIVERY SCHEDULE 

IN WITNESS whereas the parties hereto have caused this Agreement to be executed on the day and year first above written.

Signed, Sealed and Delivered by the 

Said, ……………………….. (for the Purchaser)

In the presence of ……………..

Singed, Sealed and Delivered by the 

Said ………………………. (for the Supplier)

In the presence of ……………..

NOTE : To be executed on Rs. 100/- Non-Judicial stamp paper.

4.  PERFORMANCE SECURITY FORM

To ________ (Name of the Purchaser)

Applicable to the State Bank of India and other Scheduled Banks approved in terms of the Government of India.  Ministry of Finance, Office Memorandum No. F(27)-F-1/54 dated the 25th February, 1995 for guarantee without deposit of securities upto prescribed limit.
WHERE AS ……………………. (Name of Supplier) (herein after called “the Supplier”) has undertaken, in pursuance of contract No. ………… dated…….. to supply . ………… (Description of Materials/equipment and Services)

(herein after called “the Contract”).

AND WHEREAS it has been stipulated by you in the said contract that the supplier will furnish you with a Bank guarantee by a recognized bank for the sum specified therein as security for compliance with the Supplier’s performance obligations in accordance with the Contract.

AND WHEREAS we have agreed to give the supplier a Guarantee :

THEREFORE WE hereby affirm that we are Guarantors and responsible to you, on behalf of the Supplier, up to total of ………………. (Amount of the Guarantee in Words and Figures) and we undertake to pay you, upon your first written demand declaring the Supplier to be in default under the Contract and without cavil or argument, any sum or sums within the limit of ………….. (Amount of guarantee) as aforesaid, without your needing to prove or to show grounds or reasons for your demand or the sum specified therein.

This guarantee is valid until the ………. Day of ……..20

Signature and Seal of Guarantors

…………………………………

Date . …………………. 

…………………………………

Address : ………………………

…………………………………

NOTE : 1) This will be executed on Rs. 100/- non-judicial stamp paper by a schedule Bank.

               2) The firm shall also furnish Agreement to the Performance Bank guarantee for availing 100% payment as shown in page no 79.

5.  MANUFACTURER’S AUTHORISATION FORM

No. ……. dated

To

Dear Sir,

SPECIFICATION No. 


We ___________________ who are established and reputable manufacturers of ________________ (Name and descriptions of materials/ equipment offered) having factories at _______________ (address of factory) do hereby authorize M/s. _________ (Name and address of Agent) to submit a bid, and sign the contract with your for the above materials/equipment manufactured by us against the above specification No. 


No company or firm or individual other than M/s. _______ are authorized to bid, and conclude the contract in regard to this business against this specific specification No.


We hereby extend our full guarantee and warranty as per clause 15 of the General conditions contract for the materials/equipment and services offered by the above firm against this specification No.

Yours faithfully,

(Name)

(Name of the manufacturer)

Note     :
This letter of authority should be on the letterhead of the manufacturer and should be singed by a person competent and having the power of attorney to bind the manufacturer. It should be included by the Bidder in its bid.

6.  PROFORMA FOR PERFORMANCE STATEMENT

Bid No. __________



Date of Opening ________

Time ________ Hours

Name of the Firm________________________________________________

	Order placed by (full address of purchaser)
	Order No. and Date
	Description and quantity of ordered equipment
	Date of completion of Delivery

	
	
	
	As per contract
	Actual

	
	
	
	
	


	Remarks indicating reasons for late delivery, if any
	Has the equipment been satisfactorily functioning ? (Attach a certificate from the Purchaser)

	
	


Signature of the Bidder ________________________

________________________

________________________

FORM –IIIA

DETAILS TO BE FURNISHED BY THE MANUFACTURER

	1. Specification No. 
	:
	

	2. Name of the Material
	:
	

	3. Bidder’s vendor Registration No. for this item and Name of the bidder
	:
	

	4. Quantity to be procured
	:
	

	5. Last date and time for submission of Bid
	:
	

	6. Date and time for opening of Bid
	:
	

	7. State whether Bid guarantee is enclosed 
	:
	Details

	8. State whether the quotation is in single part/ Two part
	:
	

	9. State whether 20% minimum quantity is quoted
	:
	Yes/No

	10. Whether willing to furnish performance B.G. @ 10% if order is placed
	:
	

	11. Details of remittance of specification cost
	:
	Rs.

DD No. 

Date

	12. Whether a local SSI unit/Local unit
	:
	

	13. Whether month wise delivery schedule indicated (And also indicate whether APCPDCL delivery schedule is accepted or not)
	:
	

	14. Prices whether Firm
	:
	

	15. Whether any other tax/duty payable. If so give details and the same is included/ not included.
	:
	Attested copies of relevant documents must be enclosed in orders of details furnished. 

	16. State whether APCPDCL terms of payment are accepted.
	:
	Yes/No

	17. Quantity offered for supply 
	:
	

	18. State whether 120 days validity offered 
	:
	Yes/No

	19. Whether sample is enclosed (if specified) 
	:
	

	
	
	

	20. Whether the material/equipment offered conforms to the relevant APCPDCL specification.
	:
	

	21. Whether you have executed orders of the APCPDCL previously for these items. (please give details)
	:
	i) P.O. No. & Date 

(ii) Description of materials 

(iii) Qty. ordered (iv) Qty. supplied (v) Name of the utility.  (vi) Remarks

	22. Similar details in respect of supplies made to other utilities
	:
	i) P.O. No. & Date 

(ii) Description of materials 

(iii) Qty. ordered (iv) Qty. supplied (v) Name of the utility.  (vi) Remarks

	23. This clause is deleted.
	
	

	24. Whether sales tax clearance certificate enclosed
	:
	

	25. Whether Income-tax clearance certificate enclosed.
	:
	

	26.  Details of annual financial turnover for last 5 years
	:
	

	27. Details of annual financial turnover with period which in equal to or more than 100% value of the materials quoted.
	
	    
Period 

From       To 

Turnover 

	28. The details of supplies made in any consecutive 12 months during last five years which is equal to or more than 40% of the quoted quantity
	
	Year wise details as per the proforma shown in page No. 66

	29. Details of type tests conducted for this material
	:
	Test report No. & Date and name of the test lab. 

	30. Deviations if any
	:
	a) Commercial      b) Technical 


Signature of the bidder 
:

Date 



: 

Seal of the firm 

:


SCHEDULE OF DEVIATION

a) TECHNICAL

	Sl. No.
	Requirements/ Equipments 
	Specification Clause No.
	Deviations
	Remarks 

	
	
	
	
	

	
	
	
	
	



It is hereby conformed that except for deviations mentioned above, the offer conforms to all the other features specified in Technical Specification Section of Volume-II of this Bid Document. 

Place :





Signature of the Bidder :

Date  : 





Name :







Business address  :

c) COMMERCIAL

	Sl. No.
	Requirements/ Equipments 
	Specification Clause No.
	Deviations
	Remarks 

	
	
	
	
	

	
	
	
	
	



It is hereby conformed that except for deviations mentioned above, the offer conforms to all the other features specified in Commercial Specification Section-I of this Bid Document. 

Place :






Signature of the Bidder :

Date  : 






Name :



        

         Business address  :

SCHEDULE ‘A’

DEPARTURE FROM SPECIFICATION.

	Sl. No.
	Reference to clause No. of this specification
	Departures 

	
	
	


Signature of the bidder
:

Date



: 








Seal of the firm


:

SCHEDULE ‘B’

MANUFACTURER’S AND PLACES OF MANUFACTURE

TESTING & INSPECTION.

	Sl.No.
	Description
	Manufacturer
	Place of manufacture
	Place of testing and inspection 

	
	
	
	
	


Signature of the bidder
:

Date



: 








Seal of the firm

:

SCHEDULE ‘C’

LIST OF SUPPLIES MADE SO FAR WITH FULL DETAILS OF GOODS SUPPLIED AND TO WHOM SUPPLIED

	Sl.No.
	Details of goods supplied 
	To whom supplied

	
	
	


SCHEDULE ‘D’

	Sl.No.
	Equipment
	Contents of Individual packages
	Weight kg
	Dimensions 

	
	
	
	
	


SCHEDULE ‘E’

	Sl.No
	.Item No.
	Description.

	
	
	


SCHEDULE ‘F’

PERFORMANCE STATEMENT

	Sl. No.
	Name and Address of authority who placed the order
	Order No. and date
	Name and description of the material 
	Quantity
	Value
	Name and address of consignee
	Due date of delivery
	Actual date of delivery 
	Despatching parti-culars

	1
	2
	3
	4
	5
	6
	7
	8
	9
	10

	
	
	
	
	
	
	
	
	
	


Note : 1. Attested copies/Notarized documents  of purchase orders shall be enclosed.

           2. For item No.9 of the above, Form-13 or Invoice copies ( Attested/Notarized) 


  shall be enclosed as a proof.

SIGNATURE OF THE TENDERER 

SCHEDULE – G

DETAILS OF TESTING FACILITIES

	S.No
	Name of test
	Details of testing facilities available
	Remarks

	1
	Test of raw materials

a).

b).


	
	

	2
	Routine tests

a).

b).


	
	

	3
	Acceptance tests

a).

b).


	
	

	4
	Type tests

a).

b).


	
	








Name of the firm
:







Name and signature 








of the Bidder

:







Designation

:







Date


:

SCHEDULE – H

PROFORMA FOR ELECITING INFORMATION AND APPRAISAL OF FIRM CAPABILITY AND CAPACITY TO MAUFACTURE ITEM (S) EQUIPMENT AS PER REQUIREMENT OF TENDER ENQUIRY

1)
a)
i)
Name of the tendering Firm.

ii) Complete address of the officer.

iii) Telegraphic address.

iv) Telex number.

v) Fax number.

b)
i)
Names of two responsible officers with designation (Managing 

Director / Partner / Chief General Manager / Works Engineer etc.,.)

ii) Day on which weekly holiday is observed.

a) Complete address of the works :

i) Telegraphic address

ii) Telephone Number (s)

iii) Telex number

iv) Fax number

v)
Names of two responsible officers with designation (Managing  

Director / Partner / Chief General Manager / Works Engineer etc.,

vi) Day on which weekly holiday is observed. 

d)
Names, address and telephone numbers of the references having facilities of PT Tele phones.

a)
i)
Name




Tel.No.


ii)
Address



Tel.No.

b)
i)
Name




Tel.No.


ii)
Address



Tel.No.

2) Year of Establishment

3) Construction of the Firm :

a) Private on public limited

b) Registered under the companies Act on any other Act. Give Registration No.& Date.

4) Financial position (Area & Value)

a)
i)
Land 

ii) Building (Covered area & value)

iii) Plant and machinery

iv) Total drawing limit from banks

b)
Annual financial turnover (duly audited for the last two years)

c) Latest income tax clearance certificate. 

5) Manpower 

a) Graduate Engineers.

b) Diploma Holders

c) Skilled workers

d) Unskilled workers

6) Production capacity per month of the item covered in your quotation and justification for assessment.

a) Details of plant machinery installed (places attach separate sheets, if necessary)

b) Details of raw material required

c) Source of raw material

d) Stock in hand

e) In case any raw materials are required to be imported, indicate arrangement of raw procurement.

f) Quality controls exercised in procurement of materials.

7) a) 
Details of manufacturing process 

b)
Scheme of quality controls

i) During manufacturing process

ii) At the finished stage

iii) Whether any record is being maintened in respect of quality controls exercised.

8) Details of orders executed/under execution during the last three years.

a) State Electricity Board/State Govt./Govt. of India & their Institution under takings.

b) Other important customers.

9) a)
Whether items offered conforms to IS or any other internationally recognised standards, if so, give reference. 

b)
Whether the firm is licensed to use ISI mark or any other Govt. quality mark (copies of latest test certificates issued by Govt. laboratories/any recognised test house be attached). 

10) Whether the firm has any ISO certificates (copy shall be enclosed)

Signature of the Authorised

Signatory of the firm

Seal of the firm

Note : 1. Please attach additional sheets, where required.


2. Copies of documents attached with the proforma should be attested by the firms authorised representative with stamp mark of the firm.



ANDHRA PRADESH CENTRAL POWER DISTRIBUTION CORPORATION. LIMITED

VIJAYAWADA

VENDOR  DEVELOPMENT  CELL

Letter No. CGM/P&MM/CPDCL/VR/DyEE-    /D.No.

/24, dt.      –     - 24
From

The Chief General Manager/P&MM

APCPDCL

VIJAYAWADA – 520008
To

M/s.

Dear Sir,

Sub
:
Registration – Registration of Vendors with APCPDCL for supply of……………………………………………………………… ………………………………………………………………………


Ref

:
Your letter No. …………………………………………...         
dt. …………………… 

* * *


As requested in the reference cited, necessary application form for registration of vendors with CPDCL of A.P. Ltd., is herewith enclosed. The form may be duly filled in and sent to the Chief General Manager/P&MM/ CPDCL/ VIJAYAWADA  within 30 days from the date of issue of this application .

Note
:
Please intimate the nearest railway station for the halt of express train and the distance from railway station to the factory or the bus route from the nearest railway station to the factory. 

Yours faithfully

CHIEF GENERAL MANAGER/P&MM
APCPDCL::VIJAYAWADA
INSTRUCTIONS

1. You are advised to read carefully the following instructions and also the application form completely before filling in the blanks.

2. The blanks in the application form should preferably be typed neatly against the space provided and where the space is found not sufficient, additional typed sheets may be attached giving reference to the item No. in the application.

3. The form should be signed by Proprietor/Managing Partner/Director (sitting) Commercial Manager only as the case may be who should have the authority to offer quotations and accept amendments etc., delegated by the organization management NO “ For signature” are accepted. 

4. Write your address in block letter along with your pin code No.

5. The bank account referred should be the same one through which the firm carries on majority of commercial transaction and may also be the bank through which the firm will have all business transactions with APCPDCL. 

6. The name referred to in application shall have authority to carry on business transactions with APCPDCL and APCPDCL will not entertain correspondence relating to offers from  any other person generally.

7. Please make sure the copies of certificates and documents specified in the application attested by competent authority as specified vide item (3) above are attached. This will help in quick processing of your application.

8. Incomplete or false information would render the vendor’s application liable for rejection without assigning any reason.

9. Please enclose attested copies of type test certificates as per relevant IS for the material to be registered. 

10.      Declaration

“we do hereby declare that the owners of the firm have no relationship with any firm owned/promoted by any black listed firm in any power utility, and we will agree to terminate contract if information furnished in this  regard is found false at a later date”.

ANDHRA PRADESH CENTRAL POWER DISTRIBUTION CORPORATION. LIMITED

VIJAYAWADA

FORM OF APPLICATION FOR ENLISTMENT AS APPROVED VENDOR

(MANUFACTURING UNIT)


Instructions contained on the overleaf of the APCPDCL letter for the guidance of the applying vendors should be read carefully before filling in this form.

	1. Name of the Firm
	

	2. a) Name of the material for which registration is sought
	

	b) Period from which the factory is under production
	

	3. a) 

i) Works
	Address
	Tel No.
	Telex/ Fax
	Grams

	ii) Head Office
	
	
	
	

	iii) Branches
	
	
	
	

	D.D. No. ………………….
	Date ……….. for Rs. ……………. Drawn on (Bank) ……………………………………………. ……………………………………………………. …………………………………………………….



	b) Name and address of Proprietor/Partners Directors of the Firm/Company


	

	c) Name of the sitting Director of Managing Partner

Telephone No.
	

	d) The person competent to enter into the contract or sign important communications/ Documents which will legally bind the vendor (Authority to be furnished)
	

	4. a) Is your firm incorporated under the company law?
	

	b) Is your firm registered under the Indian Partnership Act, 1932? If so, registration No. and date
	

	c) Is your factory registered under the Indian Factories Act, 1948? If so, Registration No. and Date
	

	5. Does your firm come under the scope of the industries Development and Regulations Act. 1951 and if so, give number and date of registration or license held under the Act. 
	

	6. Please state the category of establishment (viz small scale, Medium Scale or Large Scale or Cottage industry and registered as such with the director of industries of the State. If registered with the Director of Industries, please state upto what period and for what material the registration has been done (please enclose a copy of registration certificate)
	

	7. Please confirm that the equipment/material for which registration is sought confirms to relevant ISS/ Boards specifications and drawings. 
	

	8. Plant and equipment available for manufacture of material for which registration is sought. (Full details to be given)
	

	9. Skilled manpower

i) Production

ii) Design and Development 

iii) Inspection
	

	10 a) Licensed capacity

     b) Manufacturing capacity (installed)
	

	11. Last year’s capacity  utilization
	

	12. Production in the last three years (quantity and value year wise)
	

	13. Product range (list of important product)


	

	14. i) Testing and inspection facilities (Details to be furnished) please confirm that the facilities available are adequate to carry out the tests required under the relevant I.S.S.
	

	ii) Whether the products are tested to any standard specification. If so a, latest copy of test certificate any be enclosed. 
	

	15. Indicate the major raw materials used and their sources. If obtained from Govt. are there any constraint?
	

	16. Name and address of your bankers stating the name in which the accounts stands
	

	17 a) Have you executed orders of the Discoms/AP TRANSCO previously for this item. If so please give full details about the execution of orders and pending orders if any.
	

	17. b) Similar details in respect of supply to other Electricity Boards may also be furnished


	

	18. Are you on the list of approved vendors of any other organizations like D.G.S. & D, Railways and other Electricity Boards ? If so give details


	

	19. a) Did you apply for registration with the AP TRANSCO/Discoms before under this or any other item? if so, give details


	

	b) Are you already doing business with this AP TRANSCO/Discoms under some other name? If so, under what name?
	

	20. List of certificates or documents attached to this application.

(Please state whether attached or not)
	

	a) Power of attorney and copies there of
	

	b). Income Tax, Sales Tax, Turnover, Tax clearance certificate of applicant firm.
	

	c) A certificate copy of the partnership deed.
	

	d) Declaration authorizing Branch Managers to enter into contractual obligation
	

	e) Any other documents attached.
	

	21. Has the form been properly singed as required in para (3) of the instructions

(State Yes or No)
	

	22. Are the owners/partners related to any employee of the AP TRANSCO/Discoms if so, provide full details.

23. Latest CC Charges Bill with SC No and connected load.
	

	24. Organisation Chart

25. Factory Lay out

26. Income Tax/GST Registration and clearance certificate.

27. Ownership/Partnership/ Rental Deed

28. Documents indicating power of attorney/Authorised Signatory – Memorandum & Articles of Association.

29. Quality Assurance Plan.

30. Latest financial status.

31.      Declaration

“ we do hereby declare that the owners of the firm have no relationship with any firm owned/promoted by any black listed firm in any power utility, and we will agree to terminate contract if information furnished in this  regard is found false at a later date”.


	







Signature 



Name 



( in Capital Letters)



Designation 

SECTION – VIII

GENERAL & ELIGIBILITY

1.
The specification covers the design, manufacture, testing, delivery of the material as detailed in the schedule attached to the specification.

2.
ELIGIBILITY :


Imp Note:- All the certificates/ documents enclosed to the tender shall be attested or notarized. 


The tenderer who complies the following conditions need only quote.

2.1. The tenderer should quote minimum 20% of the tendered quantity.


The   bidder   should   be   a   manufacturer / registered vendor who   must   have   designed, manufactured, tested and supplied to power utilities at least 40% of the quoted quantity of the goods / equipment of same or higher voltage/capacity class indicated in the “Schedule of Requirement” in one continuous period of 12 months and its financial turnover during any one year of the last five years should have been equal or more than 100% value of the material now quoted.




 For this purpose Order completion certificates, Performance certificates issued by the utility not below the rank of General Manger / Superintending Engineer, Stores material receipt acknowledgement (Form-13) will be considered.
At least 20% of same or similar material offered against this Specification should be in successful operation since 2 years as on the date of opening of the Bid for major materials like PTRs, DTRs, VCBs, Energy Meters of all types, Instrument Transformers, Over Head Conductors / Cables, UG Cables and other equipment on the material supplied during last seven years  (and)
 since 1 year for all other materials on the material supplied during last  five years.

The requirement of 20% Performance on the same or similar material offered against the specification is based on the material to be procured 
For this purpose Performance certificates issued by the utility not below the rank of General Manger / Superintending Engineer during the last seven/five  years as on the date of opening of the Bid will only be considered.
2.2. In support of the above statement, attested copies of both purchase order and performance certificates/Form-13 from the purchasers should be enclosed .It may be noted that certificates/documents shall be attested by Gazetted officer or notarized. If the above documents/certificates are not attested or notarized,  the information given in the statement will be treated as not furnished. 

2.3. The tenderer should submit type test certificates as per relevant IS standards tested in any one of the accredited National Test Laboratories, which shall not be later than 5 years  subject no alteration in the design.   The bids received without type test reports will be treated as non-responsive “if any change in design was made latest type tests shall be furnished along with approved drawing”.
Important Note :


If the tenderer who do not comply any one of the conditions (or) do not furnish the information and the given information proved not correct their tender will be rejected and Bid Security will be forfeited. 

The tenderer should also furnish reports on financial standing such as profit and loss statements, balance sheets, auditors report for past thee years and bankers certificates etc to prove their financial capability.

3.         Filling up of schedules :

All the schedules should be duly filled in but not necessarily in the same sheets attached to the specification. Unless full details required in the schedules are furnished, offers will not be considered. 

4.       Clearing of doubts

If the bidder have any doubt about the meaning of any portion of this specification, he should at once obtain the required clarifications/ information in writing from the Chief General Manager/(P&MM)/ CPDCL/ VIJAYAWADA.

5.        BID SECURITY : 

Refer clause 20 of General and financial terms and conditions for supply of materials. Tenders with partial payment of BID SECURITY are summarily rejected

6.        DELIVERY :

The delivery shall commence within 30 days (as applicable) from the date of receipt of purchase order.

The quantities that can be delivered per month from the date of commencement of delivery shall be indicated.

The total quantity mentioned is to be supplied during the year to suit APCPDCL’s requirement. 

7.        GUARANTEE :

The material should be guaranteed for satisfactory operation as per clause 53 of Section-I from the date of receipt of material at destination stores in good condition. If during the guarantee period the material while in its normal operation is found defective it shall be replaced or rectified by the supplier within 15 days free of cost.  
CHIEF GENERAL MANAGER 

P&MM:APCPDCL::VIJAYAWADA 
SECTION - IX

AGREEMENT
PERFORMANCE BANK GUARANTEE
FOR AVAILING 100% PAYMENT

Whereas the Andhra Pradesh Central Power Distribution Corporation Limited,Vijayawada hereinafter called “The APCPDCL” has afforded a facility to persons whose tenders are accepted for the supply of materials for furnishing Performance guarantee Deposit to the extent of 10% of the value of orders on the supplies, in the shape Bank guarantee for the satisfactory fulfillment of the terms and conditions of purchase order to enable supplier to draw payment for 100% value of supplies. Whereas we ……………. (Co’s Name and full address) hereinafter called the supplier intend to avail the said facility and do hereby furnish the fixed deposit of Rs. ……….. (Rupees ……………. only) in the shape of Bank guarantee vide BG.No………………………………… dt:………….. of the ……………. (Bankers name and full address) issued by ……….Bank Ltd against the Purchase Order No…………………. dt:……………

IT IS HEREBY AGREED AND DECLARED AS FOLLOWS

1. The Bank Guarantee furnished herewith shall be valid  so as to cover performance guarantee period over and above 6 months from the date of expiry of guarantee period as per purchase order, subject to the condition that if required the Bank Guarantee should be got renewed by the supplier two months before its expiry to cover the 10% value of supplies made for which the performance guarantee period (or similar stipulation in the purchase order) has not expired on the date of expiry of the initial bank guarantee. If the bank guarantee is not renewed by the stipulated date as stated above, the APCPDCL reserves the right to operate on the subsisting bank guarantee to retain an amount equivalent to 10% of the value of supplies made for which the performance guarantee period has not expired.

2. So long  as the Bank guarantee is in force, no separate deposit is required for drawing full payments for 100% value of supplies rendered for that particular order. 

3. If there is any default on the part of the supplier from proper fulfillment of order the APCPDCL shall have the unilateral right to call upon the bank and /or supplier to forthwith pay to the APCPDCL a sum equivalent to the damages or loss sustained by the APCPDCL by reason of such default or defaults.

4. Where any such amounts have been claimed from and paid by the bank, the APCPDCL shall not be bound to permit any such supplier from non payment of deposit according to rules, in respect of the supplies unless the bank guarantee has been restored to the required level for enabling the supplier to draw the 100% value of supplies rendered. 

Dated :






Name of the Company

Place : 






With signature and stamp

Note : This should be furnished on Rs. 100/- Non-Judicial stamp paper by the Company.

SECTION - X

ACRONYMS

------------------------------------------------------------------------------------------------

Reference Abbreviations

Name and Address

------------------------------------------------------------------------------------------------

IEC



International Electro Technical





Commission Bureau Central de la





Commission Electro Technique





International, Rue de verembe





Geneva, Switzerland.

ISO



International Organisation for





Standardisation,





Danish Board of Standardisation





Aurehoegyej-12





DK-2900, Heel prup,





DENMARK

ISS



Indian Standard Bureau of 





Indian Standards





Nanak Bhavan,





9, Bahadur Shah Zafar Marg,





NEW DELHI - 110 002, INDIA

CBIP



Central Board of Irrigation and Power





Malcha Marg, Chankyapuri, 





NEW DELHI – 110 021





INDIA.

deg.C.



degrees centigrade

max.



maximum

accn.



acceleration

dB



decibels

min.



minimum

mm



millimeter

cm



centimeter

------------------------------------------------------------------------------------------------








TENDER SPECIFICATION 





CPMPT- 08/2024-25





FOR








11KV Polymer Pin Insulators with GI Pins











� EMBED Package ���





� EMBED Package ���
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67





Encl : Application form
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